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NEC3 Supply Contract (SC3)






	Between


	ESKOM HOLDINGS SOC Ltd 
(Reg No. 2002/015527/30)

	and


	[Insert at award stage]
(Reg No. ___________)

	for


	SUPPLY & DELIVERY OF VARIOUS CLASSES OF TRUCKS TO THE DISTRIBUTION GAUTENG CLUSTER ON AN AS-AND-WHEN-REQUIRED BASIS FOR A PERIOD OF THREE (3) YEARS
Insert title of the goods and services

	
	

	Contents:

	
	No of pages

	Part C1
	Agreements & Contract Data
	25

	Part C2
	Pricing Data
	4

	Part C3
	Scope of Work
	10

	
	
	

	CONTRACT No.
	[Insert at award stage]
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	Contents:

	
	No of pages

	C1.1
	Form of Offer and Acceptance 

[to be inserted from Returnable Documents at award stage]
	3

	C1.2a
	Contract Data provided by the Purchaser
	14

	C1.2b
	Contract Data provided by the Supplier

[to be inserted from Returnable Documents at award stage]
	1

	C1.3
	Proforma Guarantees
	6



ESKOM HOLDINGS SOC Ltd.		CONTRACT NUMBER ______________
SUPPLY & DELIVERY OF VARIOUS CLASSES OF NEW TRUCKS & NEW HEAVY-DUTY SINGLE-CAB 4X4 LIGHT DELIVERY VEHICLES ON “AN AS & WHEN” REQUIRED BASIS FOR THE PERIOD OF 3 YEARS AT GAUTENG CLUSTER
ESKOM HOLDINGS SOC Ltd		CONTRACT NUMBER _________
SUPPLY & DELIVERY OF VARIOUS CLASSES OF NEW TRUCKS & NEW HEAVY-DUTY SINGLE-CAB 4X4 LIGHT DELIVERY VEHICLES ON “AN AS & WHEN” REQUIRED BASIS FOR THE PERIOD OF 3 YEARS AT GAUTENG CLUSTER		



PART C1: AGREEMENT & CONTRACT DATA	PAGE 1	C1.2A SC3 CONTRACT DATA PART 1


CONTRACT	- II -	SC3 COVER PAGES

C1.1 Form of Offer & Acceptance

[bookmark: _Toc242091063]Offer

The Purchaser, identified in the Acceptance signature block, has solicited offers to enter into a contract for the procurement of:

[bookmark: _Toc242091064]Supply & Delivery of Various Classes of Trucks to the Gauteng Cluster on an as-and-when-required basis for a period of three (3) years

The tenderer, identified in the Offer signature block, has

	either
	examined the documents listed in the Tender Data and addenda thereto as listed in the Returnable Schedules, and by submitting this Offer has accepted the Conditions of Tender.

	or
	examined the draft contract as listed in the Acceptance section and agreed to provide this Offer.



By the representative of the tenderer, deemed to be duly authorised, signing this part of this Form of Offer and Acceptance the tenderer offers to perform all of the obligations and liabilities of the Supplier under the contract including compliance with all its terms and conditions according to their true intent and meaning for an amount to be determined in accordance with the conditions of contract identified in the Contract Data. 


	
	The offered total of the Prices exclusive of VAT is 
	Rates Based

	
	Value Added Tax @ 15% is
	Rates Based

	
	The offered total of the amount due inclusive of VAT is[footnoteRef:1] [1:  This total is required by the Purchaser for budgeting purposes only.  Actual amounts due will be assessed in terms of the conditions of contract.] 

	Rates Based

	
	Rates Based




This Offer may be accepted by the Purchaser by signing the Acceptance part of this Form of Offer and Acceptance and returning one copy of this document including the Schedule of Deviations (if any) to the tenderer before the end of the period of validity stated in the Tender Data, or other period as agreed, whereupon the tenderer becomes the party named as the Supplier in the conditions of contract identified in the Contract Data.

	Signature(s)

	
	
	

	Name(s)

	
	
	

	Capacity

	
	
	

	For the tenderer:

	

	
Name & signature of witness
	(Insert name and address of organisation)
	
	

Date
	

	
	



[bookmark: _Toc242091065]Acceptance

By signing this part of this Form of Offer and Acceptance, the Purchaser identified below accepts the tenderer’s Offer.  In consideration thereof, the Purchaser shall pay the Supplier the amount due in accordance with the conditions of contract identified in the Contract Data.  Acceptance of the tenderer’s Offer shall form an agreement between the Purchaser and the tenderer upon the terms and conditions contained in this agreement and in the contract that is the subject of this agreement.

The terms of the contract, are contained in: 

Part C1		Agreements and Contract Data, (which includes this Form of Offer and Acceptance)

Part C2		Pricing Data

Part C3		Scope of Work:  Goods Information including Supply Requirements

and drawings and documents (or parts thereof), which may be incorporated by reference into the above listed Parts.

Deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Returnable Schedules as well as any changes to the terms of the Offer agreed by the tenderer and the Purchaser during this process of offer and acceptance, are contained in the Schedule of Deviations attached to and forming part of this Form of Offer and Acceptance.  No amendments to or deviations from said documents are valid unless contained in this Schedule.

The tenderer shall within two weeks of receiving a completed copy of this agreement, including the Schedule of Deviations (if any), contact the Purchaser’s agent (whose details are given in the Contract Data) to arrange the delivery of any securities, bonds, guarantees, proof of insurance and any other documentation to be provided in terms of the conditions of contract identified in the Contract Data at, or just after, the date this agreement comes into effect.  Failure to fulfil any of these obligations in accordance with those terms shall constitute a repudiation of this agreement.

[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Notwithstanding anything contained herein, this agreement comes into effect on the date when the tenderer receives one fully completed and signed original copy of this document, including the Schedule of Deviations (if any).  


	Signature(s)

	
	
	

	Name(s)
	

	
	

	Capacity

	
	
	

	for the Purchaser

	
Eskom Holdings SOC Ltd, Megawatt Park, Maxwell Drive, Sandton, Johannesburg, 2199

	
Name & signature of witness
	(Insert name and address of organisation)
	
	

Date
	



Note: If a tenderer wishes to submit alternative tenders, use another copy of this Form of Offer and Acceptance.
[bookmark: _Toc242091066]
Schedule of Deviations to be completed by the Purchaser prior to contract award
Note:
1.  This part of the Offer & Acceptance would not be required if the contract has been developed by negotiation between the Parties and is not the result of a process of competitive tendering.
2. The extent of deviations from the tender documents issued by the Purchaser prior to the tender closing date is limited to those permitted in terms of the Conditions of Tender.
3. A tenderer’s covering letter must not be included in the final contract document.  Should any matter in such letter, which constitutes a deviation as aforesaid be the subject of agreement reached during the process of Offer and Acceptance, the outcome of such agreement shall be recorded here and the final draft of the contract documents shall be revised to incorporate the effect of it.

	No.
	Subject
	Details

	1
	[●]
	[●]

	2
	[●]
	[●]

	3
	[●]
	[●]

	4
	[●]
	[●]

	5
	[●]
	[●]

	6
	[●]
	[●]

	7
	[●]
	[●]

	
	
	




By the duly authorised representatives signing this Schedule of Deviations below, the Purchaser and the tenderer agree to and accept this Schedule of Deviations as the only deviations from and amendments to the documents listed in the Tender Data and any addenda thereto listed in the Tender Schedules, as well as any confirmation, clarification or changes to the terms of the Offer agreed by the tenderer and the Purchaser during this process of Offer and Acceptance.  

It is expressly agreed that no other matter whether in writing, oral communication or implied during the period between the issue of the tender documents and the receipt by the tenderer of a completed signed copy of this Form shall have any meaning or effect in the contract between the parties arising from this Agreement. 


	
	For the tenderer:

	
	For the Purchaser


	Signature

	
	
	

	Name
	

	
	

	Capacity

	
	
	

	On behalf of
	(Insert name and address of organisation)



	
	Eskom Holdings SOC Ltd, Megawatt Park, Maxwell Drive, Sandton, Johannesburg, 2199

	Name & signature of witness
	
	
	

	
Date
	
	
	



ESKOM HOLDINGS SOC Ltd.		CONTRACT NUMBER ______________
THE SUPPLY & DELIVERY OF VARIOUS CLASSES OF TRUCKS TO THE DISTRIBUTION GAUTENG CLUSTER ON AN AS-AND-WHEN-REQUIRED BASIS FOR A PERIOD OF THREE (3) YEARS		


PART C1: AGREEMENT & CONTRACT DATA	PAGE 1	C1.1 SC3 FORM OF OFFER AND ACCEPTANCE
		

C1.2 SC3 Contract Data

[bookmark: _Toc242091067]Part one - Data provided by the Purchaser

Completion of this data in full, according to the Options chosen, is essential to create a complete contract.

	Clause
	[bookmark: _Toc242091068]Statement
	[bookmark: _Toc242091069]Data

	1
	[bookmark: _Toc242091070]General
	

	
	The conditions of contract are the core clauses and the clauses for Options 
	

	
	
	X1:		Price adjustment for inflation

	
	
	X2		Changes in the law

	
	
	X3:		Multiple currencies

	
	
	X7:		Delay damages

	
	
	X13	:	Performance bond

	
	
	X17:	Low performance damages

	
	
	Z:		Additional conditions of contract

	
	of the NEC3 Supply Contract (April 2013) [footnoteRef:2] [2:  Available from Engineering Contract Strategies Tel 011 803 3008 Fax 086 539 1902, www.ecs.co.za.] 

	(If the December 2009 edition is to be used delete April 2013 and replace by December 2013)

	10.1
	The Purchaser is (name):
	Eskom Holdings SOC Ltd (reg no: 2002/015527/30), a state owned company incorporated in terms of the company laws of the Republic of South Africa

	
	Address
	Registered office at Megawatt Park, Maxwell Drive, Sandton, Johannesburg

	
	Tel No.
	

	
	Fax No.
	

	10.1
	The Supply Manager is (name): 
	

	
	Address
	

	
	Tel
	

	
	Fax
	

	
	e-mail
	

	11.2(13)
	The goods are 
	Supply of various classes of new trucks & new heavy-duty single-cab 4x4 Light Delivery Vehicles

	11.2(13)
	The services are 
	Delivery of various classes of new trucks & new heavy-duty single-cab 4x4 Light Delivery Vehicles 

	11.2(14)
	The following matters will be included in the Risk Register
	


	11.2(15)
	The Goods Information is in 
	Part 3: Scope of Work and all documents and drawings to which it makes reference.

	11.2(15)
	The Supply Requirements as part of the Goods Information is in 
	Annexure A to this Contract Data

	12.2
	The law of the contract is the law of 
	the Republic of South Africa

	13.1
	The language of this contract is 
	English

	13.3
	The period for reply is
	1 weeks

	[bookmark: _Toc242091071]2
	[bookmark: _Toc242091072]The Supplier’s main responsibilities
	Data required by this section of the core clauses is provided by the Supplier in Part 2 and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc242091073]3
	[bookmark: _Toc242091074]Time
	

	30.1
	The starting date is.
	TBC (Date on which the contract number is issued)

	30.1
	The delivery date of the goods and services is:
	goods and services 
	delivery date

	
	
	1
	As stipulated in each purchase order
	

	30.2
	The Supplier does not bring the goods to the Delivery Place more than one week before the Delivery Date.
	

	31.1
	The Supplier is to submit a first programme for acceptance within 
	
1 week after placing an order.

	32.2
	The Supplier submits revised programmes at intervals no longer than 
	
1 week for each purchase order placed

	[bookmark: _Toc242091075]4
	[bookmark: _Toc242091076]Testing and defects
	

	42
	The defects date is 
	52 weeks after Delivery.

	43.2
	The defect correction period is 
	2 weeks

	42.2
	The defects access period is  
	5 days

	[bookmark: _Toc242091077]5
	[bookmark: _Toc242091078]Payment
	

	50.1
	The assessment interval is 
	Within 1 week of delivery date

	51.1
	The currency of this contract is the 
	South African Rand

	51.2
	The period within which payments are made is
	
4 weeks after invoice submission with a goods receipt

	[bookmark: _Toc242091079]6
	[bookmark: _Toc242091080]Compensation events
	There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc242091081]7
	[bookmark: _Toc242091082]Title
	[bookmark: _Toc242091083]There is no reference to Contract Data in this section of the core clauses and terms in italics used in this section are identified elsewhere in this Contract Data.

	[bookmark: _Toc242091084]8
	[bookmark: _Toc242091085]Risks, liabilities, indemnities and insurance
	

	80.1
	These are additional Purchaser’s risks  
	None

	88.1
	The Supplier’s liability to the Purchaser for indirect or consequential loss, including loss of profit, revenue and goodwill is limited to
	Total of purchase orders issued.


R0.0 (zero Rand)

	88.2
	For any one event, the Supplier’s liability to the Purchaser for loss of or damage to the Purchaser’s property is limited to
	(1) for the Purchaser’s existing and surrounding property in the care, custody and control of the Supplier the amount of the deductible (first amount payable) relevant to the event 
and

(2) for all other existing Purchaser’s property the applicable deductible as at contract date 
As per Annexure B, Annual Construction All Risk policy




	88.3
	The Supplier’s liability for Defects due to his design which are not notified before the last defects date is limited to:
	The total of the prices, plus the amount of the deductibles payable in respect of the Employer’s Annual Construction All Risk Insurance Policy in respect of the resultant damages caused by the defective equipment. 


	88.4
	The Supplier’s total liability to the Purchaser, for all matters arising under or in connection with this contract, other than the excluded matters, is limited to
	The total value of the defective equipment



	88.5
	The end of liability date is 
	3 years after Delivery of the whole of the goods and services.

	[bookmark: _Toc242091086]9
	[bookmark: _Toc242091087]Termination and dispute resolution
	

	94.1
	The Adjudicator is 
	the person selected from the ICE-SA Division (or its successor body) of the South African Institution of Civil Engineering Panel of Adjudicators by the Party intending to refer a dispute to him.  (see www.ice-sa.org.za). If the Parties do not agree on an Adjudicator the Adjudicator will be appointed by the Arbitration Foundation of Southern Africa (AFSA).

	
	Address
	

	
	Tel No.
	

	
	Fax No.
	

	
	e-mail
	

	94.2(3)
	The Adjudicator nominating body is: 
	the Chairman of ICE-SA, a Division of the South African Institution of Civil Engineering, or its successor body (See www.ice-sa.org.za)

	94.4(2)
	The tribunal is: 
	arbitration

	94.4(5)
	The arbitration procedure is 
	the latest edition of Rules for the Conduct of Arbitrations published by The Association of Arbitrators (Southern Africa) or its successor body.

	94.4(5)
	The place where arbitration is to be held is
	Gauteng, South Africa

	
	The person or organisation who will choose an arbitrator 
· if the Parties cannot agree a choice or
· if the arbitration procedure does not state who selects an arbitrator, is
	

the Chairman for the time being or his nominee of the Association of Arbitrators (Southern Africa) or its successor body.

	[bookmark: _Toc242091088]10
	[bookmark: _Toc242091089]Data for Option clauses
	

	X1
	Price adjustment for inflation
	

	X1.1
	The base date for indices is 
	The month before tender closing – to be updated upon contract award.

	
	The proportions used to calculate the Price Adjustment Factor are:
	proportion
	linked to index for
	Index prepared by

	
	
	0.85
	Consumer Price Index (CPI)- TABLE D-4
	SEIFSA

	
	Prices will be fixed and firm for the first 12 months of the contract. At the anniversary date of the contract the prices will be adjusted. 

	0.15
	non-adjustable
	

	
	
	1.00

	
	

	X2
	Changes in the law
	

	X2.1
	A change in the law of 

	South Africa is a compensation event if it occurs after the Contract Date

	X3
	Multiple currencies
	

	X3.1

	The Purchaser will pay for these items in the currencies stated
	
Items
	
Other currency
	Total maximum payment in the currency

	
	
	[●]
	[bookmark: Text539]     
	[bookmark: Text540]     

	
	
	[●]
	[bookmark: Text542]     
	[bookmark: Text543]     

	
	
	[●]
	[bookmark: Text545]     
	[bookmark: Text546]     

	X3.1
	The exchange rates are those published in
	[●] on [●] (date)

	
	
	The items will be paid in the other currency 
- to a foreign Bank account nominated by the Supplier 
- to a valid SARB approved CFC account in South Africa
- in accordance with an alternative payment method agreed with the Purchaser before the Contract Date.

(select one of the three methods as agreed with the successful tenderer prior to contract award and delete the others and this note)

	X7
	Delay damages
	

	X7.1
	Delay damages for Delivery are
	Delivery of
	amount per day

	
	
	Delivery lead time
	0.5% per week, capped at 10% of each order value calculated on the value of the delayed portion.

	
	
	
	

	
	
	
	

	
	
	
	

	X13
	Performance bond
	

	X13.1
	The amount of the performance bond is
	10% of the value of each Purchase Order issued under the Contract.

	X17
	Low performance damages

	


	Criteria
	Weight
	Unit
	Target
	Penalty- 5% per Task order
	Penalty- 10% per Task order
	Penalty -15% per Task order

	Rework
	45%
	Months
	0
	1
	3
	5

	SHEQ 
	20%
	Months
	0
	1
	3
	5

	Non-Conformance Report
	15%
	Per Number
	0
	1
	2
	3

	Call out response
	20%
	Hr
	2 HRS
	3 HRS
	5HRS
	7HRS

	Total
	100%
	
	
	
	
	


	Z
	The additional conditions of contract are
	
Z1 to Z15 always apply for Eskom

	
	

	Z1
	Cession delegation and assignment

	Z1.1
	The Supplier does not cede, delegate or assign any of its rights or obligations to any person without the written consent of the Purchaser.

	Z1.2
	Notwithstanding the above, the Purchaser may on written notice to the Supplier cede and delegate its rights and obligations under this contract to any of its subsidiaries or any of its present divisions or operations which may be converted into separate legal entities as a result of the restructuring of the Electricity Supply Industry. 

	
	

	Z2
	Joint ventures

	Z2.1
	If the Supplier constitutes a joint venture, consortium or other unincorporated grouping of two or more persons or organisations then these persons or organisations are deemed to be jointly and severally liable to the Purchaser for the performance of this contract.

	Z2.2
	Unless already notified to the Purchaser, the persons or organisations notify the Supply Manager within two weeks of the Contract Date of the key person who has the authority to bind the Supplier on their behalf.

	Z2.3
	The Supplier does not alter the composition of the joint venture, consortium or other unincorporated grouping of two or more persons without the consent of the Purchaser having been given to the Supplier in writing.

	
	

	Z3
	Change of Broad Based Black Economic Empowerment (B-BBEE) status

	Z3.1
	Where a change in the Supplier’s legal status, ownership or any other change to his business composition or business dealings results in a change to the Supplier’s B-BBEE status, the Supplier notifies the Purchaser within seven days of the change.

	Z3.2
	The Supplier is required to submit an updated verification certificate and necessary supporting documentation confirming the change in his B-BBEE status to the Supply Manager within thirty days of the notification or as otherwise instructed by the Supply Manager.

	Z3.3
	Where, as a result, the Supplier’s B-BBEE status has decreased since the Contract Date the Purchaser may either re-negotiate this contract or alternatively, terminate the Supplier’s obligation to Provide the Goods and Services.

	Z3.4
	Failure by the Supplier to notify the Purchaser of a change in its B-BBEE status may constitute a reason for termination. If the Purchaser terminates in terms of this clause, the procedures on termination are P1, P2 and P3 as stated in clause 92, and the amount due is A1 and A3 as stated in clause 93.

	
	

	Z4
	Confidentiality

	Z4.1
	The Supplier does not disclose or make any information arising from or in connection with this contract available to Others. This undertaking does not, however, apply to information which at the time of disclosure or thereafter, without default on the part of the Supplier, enters the public domain or to information which was already in the possession of the Supplier at the time of disclosure (evidenced by written records in existence at that time).  Should the Supplier disclose information to Others in terms of clause 23.1, the Supplier ensures that the provisions of this clause are complied with by the recipient.

	Z4.2
	If the Supplier is uncertain about whether any such information is confidential, it is to be regarded as such until notified otherwise by the Supply Manager.

	Z4.3
	In the event that the Supplier is, at any time, required by law to disclose any such information which is required to be kept confidential, the Supplier, to the extent permitted by law prior to disclosure, notifies the Purchaser so that an appropriate protection order and/or any other action can be taken if possible, prior to any disclosure.  In the event that such protective order is not, or cannot, be obtained, then the Supplier may disclose that portion of the information which it is required to be disclosed by law and uses reasonable efforts to obtain assurances that confidential treatment will be afforded to the information so disclosed.

	Z4.4
	The taking of images (whether photographs, video footage or otherwise) of the goods or any portion thereof, in the course of Providing the Goods and Services and after Delivery, requires the prior written consent of the Supply Manager.  All rights in and to all such images vests exclusively in the Purchaser.  

	Z4.5
	The Supplier ensures that all his subcontractors abide by the undertakings in this clause.

	
	

	Z5
	Waiver and estoppel: Add to core clause 12.3:

	Z5.1
	Any extension, concession, waiver or relaxation of any action stated in this contract by the Parties, the Supply Manager or the Adjudicator does not constitute a waiver of rights, and does not give rise to an estoppel unless the Parties agree otherwise and confirm such agreement in writing.

	
	

	Z6
	Health, safety and the environment:  Add to core clause 25.4

	Z6.1
	The Supplier undertakes to take all reasonable precautions to maintain the health and safety of persons in and about the provision of the goods and execution of the services. 

Without limitation the Supplier:

warrants that the total of the Prices as at the Contract Date includes a sufficient amount for proper compliance with all applicable health & safety laws and regulations and the health and safety rules, guidelines and procedures provided for in this contract and generally for the proper maintenance of health & safety in and about the execution of supply and
undertakes, in and about the execution of the supply, to comply with all applicable health & safety laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Subcontractors, employees and others under the Supplier’s direction and control, likewise observe and comply with the foregoing.

	Z6.2
	The Supplier, in and about the execution of the supply, complies with all applicable environmental laws and regulations and rules, guidelines and procedures otherwise provided for under this contract and ensures that his Subcontractors, employees and others under the Supplier’s direction and control, likewise observe and comply with the foregoing.

	
	

	Z7
	Provision of a Tax Invoice and interest.  Add to core clause 51

	Z7.1
	Within one week of receiving a payment certificate from the Supply Manager in terms of core clause 51.1, the Supplier provides the Purchaser with a tax invoice in accordance with the Purchaser's procedures stated in the Goods Information, showing the amount due for payment equal to that stated in the payment certificate.

	Z7.2
	If the Supplier does not provide a tax invoice in the form and by the time required by this contract, the time by when the Purchaser is to make a payment is extended by a period equal in time to the delayed submission of the correct tax invoice.  Interest due by the Purchaser in terms of core clause 51.2 is then calculated from the delayed date by when payment is to be made.

	Z7.3
	The Supplier (if registered in South Africa in terms of the companies Act) is required to comply with the requirements of the Value Added Tax Act, no 89 of 1991 (as amended) and to include the Purchaser’s VAT number 4740101508 on each invoice he submits for payment.

	
	

	Z8
	Notifying compensation events

	Z8.1
	Delete from the last sentence in core clause 61.3 the words, “unless the event arises from the Supply Manager giving an instruction, changing an earlier decision or correcting an assumption”.

	
	

	[bookmark: OLE_LINK5][bookmark: OLE_LINK6]Z9
	Purchaser’s limitation of liability

	Z9.1
	The Purchaser’s liability to the Supplier for the Supplier’s indirect or consequential loss is limited to R0.00 (zero Rand)

	Z9.2
	The Supplier’s entitlement under the indemnity in 83.1 is provided for in 60.1(12) and the Purchaser’s liability under the indemnity is limited.

	
	

	Z10
	Termination: Add to core clause 91.1, at the second main bullet point, fourth sub-bullet point, after the words "against it":  

	Z10.1
	   or had a business rescue order granted against it.

	
	

	Z11
	Addition to secondary Option X7 Delay damages (if applicable in this contract)

	Z11.1
	If the amount due for the Supplier’s payment of delay damages reaches the limits stated in this Contract Data for Option X7, the Purchaser may terminate the Supplier’s obligation to Provide the Goods and Services using the same procedures and payment on termination as those applied for reasons R1 to R15 or R18 stated in the Termination Table.

	
	

	Z12
	Ethics

	For the purposes of this Z-clause, the following definitions apply:

	Affected Party
	means, as the context requires, any party, irrespective of whether it is the Supplier or a third party, such party’s employees, agents, or Subcontractors or Subcontractor’s employees, or any one or more of all of these parties’ relatives or friends,

	Coercive Action
	means to harm or threaten to harm, directly or indirectly, an Affected Party or the property of an Affected Party, or to otherwise influence or attempt to influence an Affected Party to act unlawfully or illegally,

	Collusive Action
	means where two or more parties co-operate to achieve an unlawful or illegal purpose, including to influence an Affected Party to act unlawfully or illegally,

	Committing Party
	means, as the context requires, the Supplier, or any member thereof in the case of a joint venture, or its employees, agents, or Subcontractors or the Subcontractor’s employees,

	Corrupt Action
	means the offering, giving, taking, or soliciting, directly or indirectly, of a good or service to unlawfully or illegally influence the actions of an Affected Party,

	Fraudulent Action
	means any unlawfully or illegally intentional act or omission that misleads, or attempts to mislead, an Affected Party, in order to obtain a financial or other benefit or to avoid an obligation or incurring an obligation,

	Obstructive Action
	means a Committing Party unlawfully or illegally destroying, falsifying, altering or concealing information or making false statements to materially impede an investigation into allegations of Prohibited Action, and

	Prohibited Action
	means any one or more of a Coercive Action, Collusive Action Corrupt Action, Fraudulent Action or Obstructive Action.

	Z12.1
	A Committing Party may not take any Prohibited Action during the course of the procurement of this contract or in execution thereof.

	Z12.2
	The Purchaser may terminate the Supplier’s obligation to Provide the Services if a Committing Party has taken such Prohibited Action and the Supplier did not take timely and appropriate action to prevent or remedy the situation, without limiting any other rights or remedies the Purchaser has. It is not required that the Committing Party had to have been found guilty, in court or in any other similar process, of such Prohibited Action before the Purchaser can terminate the Supplier’s obligation to Provide the Services for this reason.

	Z12.3
	If the Purchaser terminates the Supplier’s obligation to Provide the Services for this reason, the amounts due on termination are those intended in core clauses 92.1 and 92.2.

	Z12.4
	A Committing Party co-operates fully with any investigation pursuant to alleged Prohibited Action. Where the Purchaser does not have a contractual bond with the Committing Party, the Supplier ensures that the Committing Party co-operates fully with an investigation.




Z13	Insurance

Z __13.1	Replace core clause 84 with the following:
	Insurance cover
	84
	

	
	84.1
	When requested by a Party, the other Party provides certificates from his insurer or broker stating that the insurances required by this contract are in force. 

	
	84.2
	The Supplier provides the insurances stated in the Insurance Table A for events which are at the Supplier’s risk from the starting date until the last defects date or a termination certificate has been issued.

	
	
	




	INSURANCE TABLE A

		Insurance against
	Minimum amount of cover or minimum limit of indemnity

	Loss of or damage to the goods, plant and materials
	The replacement cost where not covered by the Purchaser’s insurance.

The Purchaser’s policy deductible as at Contract Date, where covered by the Purchaser’s insurance.

	Liability for loss of or damage to property (except the goods, plant and materials and equipment) and liability for bodily injury to or death of a person (not an employee of the Supplier) caused by activity in connection with this contract
	Loss of or damage to property
Purchaser’s property
The replacement cost where not covered by the Purchaser’s insurance.

The Purchaser’s policy deductible as at Contract Date, where covered by the Purchaser’s insurance.

Other property
The replacement cost

Death of or bodily injury
The amount required by the applicable law.

	Liability for death of or bodily injury to employees of the Supplier arising out of and in the course of their employment in connection with this contract
	The amount required by the applicable law 






Z _13.2		Replace core clause 87 with the following:

	Insurance by the Purchaser
	
	87
	

	
	
	87.1
	The Purchaser provides the insurances stated in the Insurance Table B

	
	
	
	INSURANCE TABLE B

	Insurance against or name of policy
	Minimum amount of cover or minimum limit of indemnity

	Assets All Risk
	Per the insurance policy document

	Contract Works insurance
	Per the insurance policy document

	Environmental Liability
	Per the insurance policy document

	General and Public Liability
	Per the insurance policy document

	Transportation (Marine)
	Per the insurance policy document

	Motor Fleet and Mobile Plant
	Per the insurance policy document

	Terrorism
	Per the insurance policy document

	Cyber Liability
	Per the insurance policy document

	Nuclear Material Damage and Business Interruption
	Per the insurance policy document

	Nuclear Material Damage Terrorism
	Per the insurance policy document





	Z14
	Nuclear Liability

	Z14.1
	The Purchaser is the operator of the Koeberg Nuclear Power Station (KNPS), a nuclear installation, as designated by the National Nuclear Regulator of the Republic of South Africa, and is the holder of a nuclear licence in respect of the KNPS.

	Z14.2
	The Purchaser is solely responsible for and indemnifies the Supplier or any other person against any and all liabilities which the Supplier or any person may incur arising out of or resulting from nuclear damage, as defined in Act 47 of 1999, save to the extent that any liabilities are incurred due to the unlawful intent of the Supplier or any other person or the presence of the Supplier or that person or any property of the Supplier or such person at or in the KNPS or on the KNPS site, without the permission of the Purchaser or of a person acting on behalf of the Purchaser.

	Z14.3
	Subject to clause Z14.4 below, the Purchaser waives all rights of recourse, arising from the aforesaid, save to the extent that any claims arise or liability is incurred due or attributable to the unlawful intent of the Supplier or any other person, or the presence of the Supplier or that person or any property of the Supplier or such person at or in the KNPS or on the KNPS site, without the permission of the Purchaser or of a person acting on behalf of the Purchaser.

	Z14.4
	The Purchaser does not waive its rights provided for in section 30 (7) of Act 47 of 1999, or any replacement section dealing with the same subject matter.

	Z14.5
	The protection afforded by the provisions hereof shall be in effect until the KNPS is decommissioned.

	
	

	Z15
	Asbestos

	For the purposes of this Z-clause, the following definitions apply:

	AAIA
	means approved asbestos inspection authority.

	ACM
	means asbestos containing materials.

	AL
	means action level, i.e. a level of 50% of the OEL, i.e. 0.1 regulated asbestos fibres per ml of air measured over a 4 hour period. The value at which proactive actions is required in order to control asbestos exposure to prevent exceeding the OEL.

	Ambient Air
	means breathable air in area of work with specific reference to breathing zone, which is defined to be a virtual area within a radius of approximately 30cm from the nose inlet.

	Compliance Monitoring
	means compliance sampling used to assess whether or not the personal exposure of workers to regulated asbestos fibres is in compliance with the Standard’s requirements for safe processing, handling, storing, disposal and phase-out of asbestos and asbestos containing material, equipment and articles.

	OEL
	means occupational exposure limit.

	Parallel Measurements
	means measurements performed in parallel, yet separately, to existing measurements to verify validity of results.

	Safe Levels
	means  airborne asbestos exposure levels conforming to the Standard’s requirements for safe processing, handling, storing, disposal and phase-out of asbestos and asbestos containing material, equipment and articles.

	Standard
	means the Purchaser’s Asbestos Standard 32-303: Requirements for Safe Processing, Handling, Storing, Disposal and Phase-out of Asbestos and Asbestos Containing Material, Equipment and Articles.

	SANAS
	means the South African National Accreditation System.

	TWA
	means the average exposure, within a given workplace, to airborne asbestos fibres, normalised to the baseline of a 4 hour continuous period, also applicable to short term exposures, i.e. 10-minute TWA.

	Z15.1
	The Purchaser ensures that the Ambient Air in the area where the Supplier will Provide the Services conforms to the acceptable prescribed South African standard for asbestos, as per the regulations published in GNR 155 of 10 February 2002, under the Occupational Health and Safety Act, 1993 (Act 85 of 1993) (“Asbestos Regulations”). The OEL for asbestos is 0.2 regulated asbestos fibres per millilitre of air as a 4-hour TWA, averaged over any continuous period of four hours, and the short term exposure limit of 0.6 regulated asbestos fibres per millilitre of air as a 10-minute TWA, averaged over any 10 minutes, measured in accordance with HSG248 and monitored according to HSG173 and OESSM.

	Z15.2
	Upon written request by the Supplier, the Purchaser certifies that these conditions prevail. All measurements and reporting are effected by an independent, competent, and certified occupational hygiene inspection body, i.e. a SANAS accredited and Department of Employment and Labour approved AAIA. The Supplier may perform Parallel Measurements and related control measures at the Supplier’s expense. For the purposes of compliance the results generated from Parallel Measurements are evaluated only against South African statutory limits as detailed in clause Z15.1. Control measures conform to the requirements stipulated in the AAIA-approved asbestos work plan.

	Z15.3
	The Purchaser manages asbestos and ACM according to the Standard.

	Z15.4
	In the event that any asbestos is identified while Providing the Services, a risk assessment is conducted and if so required, with reference to possible exposure to an airborne concentration of above the AL for asbestos, immediate control measures are implemented and relevant air monitoring conducted in order to declare the area safe.

	Z15.5
	The Supplier’s personnel are entitled to stop working and leave the contaminated area forthwith until such time that the area of concern is declared safe by either Compliance Monitoring or an AAIA approved control measure intervention, for example, per the emergency asbestos work plan, if applicable.

	Z15.6
	The Supplier continues to Provide the Services, without additional control measures presented, on presentation of Safe Levels. The contractually agreed dates to Provide the Services, including the Completion Date, are adjusted accordingly. The contractually agreed dates are extended by the notification periods required by regulations 3 and 21 of the Asbestos Regulations.

	Z15.7
	Any removal and disposal of asbestos, asbestos containing materials and waste, is done by a registered asbestos contractor, instructed by the Purchaser at the Purchaser’s expense, and conducted in line with South African legislation.


Annexure A:	Supply Requirements

[Notes: The example given in the NEC3 Supply Contract Guidance Notes pages 15 to 20 inclusive is based on Incoterms 2000.   However users will probably wish to use Incoterms 2010 which the details below are based on.    Users may need to adjust the information to comply with actual requirements. First decide whether Incoterms will be used or not, then delete the arrangement below which does not apply and delete these notes]

[bookmark: _Toc242091090]The Supply Requirements for this contract are based on the use of INCOTERMS:

The Supplier supplies the goods in accordance with INCOTERMS 2010[footnoteRef:3] as follows: [3:  International Chamber of Commerce, Incoterms 2010, Paris, January 2011] 


[Select the group and then term within the group which applies and state the applicable delivery place.  Delete all the other groups and this note]

	Group
	Category
	Term
	Delivery Place

	E
	departure
	EXW
	

	F
	main carriage unpaid
	FCA, FAS, FOB
	

	C
	main carriage paid
	CFR, CIF, CPT, CIP
	

	D
	arrival
	DAT, DAP, DDP
	



The Parties obligations described in Incoterms for the category and term selected are now incorporated into this contract as part of the Supply Requirements and hence the Goods Information.  

The obligations of seller and buyer for the selected Incoterm determine each Party's costs, risks and insurance requirements incidental to the supply and transport of the goods from Supplier to Purchaser.

For each of the thirteen terms, Incoterms set out obligations of the seller (the Supplier) in ten paragraphs identified as A1 to A10 and the corresponding obligations of the buyer (the Purchaser) in paragraphs B1 to B10.  These obligations cover the following subjects:

	A
	The Supplier’s obligations
	B
	The Purchaser’s obligations

	A1
	Provision of goods in conformity with contract
	B1
	Payment of the price

	A2
	Licences, authorisations and formalities
	B2
	Licences, authorisations and formalities

	A3 
	Contracts of carriage and insurance
	B3
	Contracts of carriage and insurance

	A4
	Delivery
	B4
	Taking delivery

	A5
	Transfer of risks
	B5
	Transfer of risks

	A6 
	Division of costs
	B6
	Division of costs

	A7
	Notice to the buyer 
	B7
	Notice to the seller

	A8
	Proof of delivery, transport document or equivalent electronic message
	B8
	Proof of delivery, transport document or equivalent electronic message

	A9
	Checking - packing - marking
	B9
	Inspection of goods

	A10
	Other obligations
	B10
	Other obligations



[Should there be a need to amplify any of the published obligations listed above for the chosen INCOTERM, add them here.]

All other information NOT pertinent to the above is given in the balance of the Goods Information
[bookmark: _Toc242091091]
The Supply Requirements for this contract are as follows:
[Use these when INCOTERMS do not apply].  [Revise and complete as required]

	1. The requirements for the supply are
	[State the constraints on how the Supplier manufactures, prototypes, tests and stores the goods including order and timing]

	2. The requirements for transport are 
	[State the extent to which the Supplier transports the goods and the mode of transport]

	3. The delivery place is
	[State the location where the goods are to be placed by the Supplier, such as whether it is a dispatch department at the Supplier’s premises, the Purchaser is to collect or other location the Purchaser may require. If the delivery place for the services is different to the goods state it here]

	4. Actions of the Parties during supply
	Action
	Party which does it

	
	Giving notice of Delivery
	

	
	Checking packing and marking before dispatch
	

	
	Contracting for transport
	

	
	Pay costs of transport
	

	
	Arrange access to delivery place
	

	
	Loading the goods
	

	
	Unloading the goods
	

	For international procurement
	Undertake export requirements
	

	
	Undertake import requirements
	

	5. Information to be provided by the Supplier 
	Title of document

	
	Packing lists for cases and their contents

	
	Copy of invoice for the goods

	
	Delivery Note

	
	Test results and maintenance manuals

	For  international procurement
	Licences, authorisations and other formalities associated with export of the goods 

	
	Air Waybill or Bill of Lading with associated landing, delivery and forwarding order 

	
	The Bill of Entry endorsed by the importation authority

	
	Customs work sheets, showing tax, duties and surcharges which the law of the country into which the goods are being imported requires the importer to pay

	
	Invoice from the importation clearing agent showing airline fees, landing charges, wharfage and dock dues as applicable

	
	Specify other import documents required by authorised officials. 
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[bookmark: OLE_LINK3][bookmark: OLE_LINK4]
C1.2 Contract Data

[bookmark: _Toc242091092]Part two - Data provided by the Supplier

Completion of the data in full, according to Options chosen, is essential to create a complete contract.

	[bookmark: _Toc242091093]Clause
	[bookmark: _Toc242091094]Statement
	[bookmark: _Toc242091095]Data

	10.1
	The Supplier is (Name):
	

	
	Address
	

	
	Tel No.
	

	
	Fax No.
	

	11.2(8)
	The Goods Information for the Supplier’s design is in:
	
This contract, Part 3

	11.2(11)
	The tendered total of the Prices is
	Rate Only

	11.2(12)
	The price schedule is in:
	Pricing Data

	11.2(14)
	The following matters will be included in the Risk Register
	


	25.2
	The restrictions to access for the Supply Manager and Others to work being done for this contract are
	



	30.1
	The delivery date of the goods and services is:
	
goods and services 
	
delivery date

	
	
	1
	Supply & delivery of various classes of new trucks & new heavy-duty single-cab 4x4 Light Delivery Vehicles
	4 to 6 weeks from the receipt of the Purchase order

	31.1
	The programme identified in the Contract Data is contained in:
	


	63.2
	The percentage for overheads and profit added to the Defined Cost is
	[bookmark: Text453]
%
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C1.3 Forms of Securities 



[bookmark: _Toc242091096]Pro formas for Bonds & Guarantees

[bookmark: _Toc242091097]For use with the NEC3 Supply Contract (SC3)



The conditions of contract stated in the Contract Data Part 1 may include the following Options:

Option X13:	Performance bond

These Options require a bond or guarantee “in the form set out in the Goods Information”. 
Pro forma documents for these bonds and guarantees are provided here for convenience but are to be treated as part of the Goods Information.



The organisation providing the bond / guarantee does so by copying the pro forma document onto it’s letterhead without any change to the text or format and completing the required details.  The completed document is then given to the Purchaser within the time stated in the contract.  




[bookmark: _Toc242091100]Pro forma Performance Bond – Demand Guarantee (for use with Option X13)
(to be reproduced exactly as shown below on the letterhead of the Bank providing the Bond / Guarantee)

	Eskom Holdings SOC Ltd
Megawatt Park
Maxwell Drive
Sandton	
Johannesburg
	Bank reference No.



	

	
	Date:
	



Dear Sirs,

Performance Bond – Demand Guarantee for [insert name of Supplier] required in terms of contract [insert Supplier’s contract reference number or title]

1. [bookmark: _Toc101080804]In this Guarantee the following words and expressions shall have the following meanings:-

	1.1
	“Bank” means
	[Insert name of Bank], [●] Branch, Registration No. [●]

	1.2
	“Bank’s Address” means
	[Insert physical address of Bank]

	1.3
	“Contract” means
	the written agreement relating to providing the goods and services, entered into between the Purchaser and the Supplier, on or about the [●] day of [●] 200[●] (Contract Reference No. [●]) as amended, varied, restated, novated or substituted from time to time; 

	1.4
	“Supplier” means
	[●] a company registered in accordance with the laws of [●] under Registration No [●].

	1.5
	“Purchaser” means
	Eskom Holdings SOC Ltd a company registered in accordance with the laws of the Republic of South Africa under Registration Number [●]

	1.6
	“Expiry Date” means
	the earlier of

· the date that the Bank receives a notice from the Purchaser stating that all amounts due from the Supplier as certified in terms of the contract have been received by the Purchaser and that the Supplier has fulfilled all his obligations under the Contract, or
· the date that the Bank issues a replacement Bond for such lesser or higher amount as may be required by the Purchaser.

	1.7
	“Guaranteed Sum” means
	the sum of R[●], ([●] Rand)

	1.8
	“goods and services” means
	[insert details from Contract Data part 1]



2. [bookmark: _Toc101080805][bookmark: _Toc101080806]At the instance of the Supplier, we the undersigned ______________ and ______________, in our respective capacities as _____________ and ___________ of the Bank, and duly authorized thereto, confirm that we hold the Guaranteed Sum at the disposal of the Purchaser as security for the proper performance by the Supplier of all of its obligations in terms of and arising from the Contract and hereby undertake to pay to the Purchaser, on written demand from the Purchaser received prior to the Expiry Date, any sum or sums not exceeding in total the Guaranteed Sum.

3. [bookmark: _Toc101080807][bookmark: _Ref138050677]A demand for payment under this guarantee shall be made in writing at the Bank’s address and shall:

· be signed on behalf of the Purchaser by a Group Executive, Divisional Executive, Senior General Manager, General Manager or its delegate;
· state the amount claimed (“the Demand Amount’);
· [bookmark: _Ref138050694]state that the Demand Amount is payable to the Purchaser in the circumstances contemplated in the Contract.

4. [bookmark: _Toc101080809]Notwithstanding the reference herein to the Contract the liability of the Bank in terms hereof is as principal and not as surety and the Bank’s obligation/s to make payment:

· is and shall be absolute provided demand is made in terms of this bond in all circumstances; and
· is not, and shall not be construed to be, accessory or collateral on any basis whatsoever. 

5. [bookmark: _Toc101080810]The Bank’s obligations in terms of this Guarantee:

· shall be restricted to the payment of money only and shall be limited to the maximum of the Guaranteed Sum; and
· shall not be discharged and compliance with any demand for payment received by the Bank in terms hereof shall not be delayed, by the fact that a dispute may exist between the Purchaser and the Supplier.

6. [bookmark: _Toc101080811]The Purchaser shall be entitled to arrange its affairs with the Supplier in any manner which it sees fit, without advising us and without affecting our liability under this Guarantee. This includes, without limitation, any extensions, indulgences, release or compromise granted to the Supplier or any variation under or to the Contract. 

7. [bookmark: _Ref139444068]Should the Purchaser cede its rights against the Supplier to a third party where such cession is permitted under the Contract, then the Purchaser shall be entitled to cede to such third party the rights of the Purchaser under this Guarantee on written notification to the Bank of such cession.

8. [bookmark: _Toc101080812]This Guarantee:

· shall expire on the Expiry Date until which time it is irrevocable;
· is, save as provided for in 7 above, personal to the Purchaser and is neither negotiable nor transferable;
· shall be returned to the Bank upon the earlier of payment of the full Guaranteed Sum or expiry hereof;
· shall be regarded as a liquid document for the purpose of obtaining a court order; and
· shall be governed by and construed in accordance with the law of the Republic of South Africa and shall be subject to the jurisdiction of the Courts of the Republic of South Africa. 
· will be invalid and unenforceable if any claim which arises or demand for payment is received after the Expiry Date.

9. [bookmark: _Toc101080813]The Bank chooses domicilium citandi et executandi for all purposes in connection with this Guarantee at the Bank’s Address.

	Signed at
	
	on this
	
	day of 
	
	20__



For and on behalf of the Bank

	Bank Signatories(s)
	
	

	Name(s) (printed)
	
	

	Witness(s)

	
	

	Bank’s seal or stamp
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[bookmark: _Toc242091101]Part 2: Pricing Data
NEC3 Supply Contract










	Document reference
	Title
	No of pages

	C2.1
	Pricing assumptions
	2

	C2.2
	The price schedule 
	1
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C2.1 Pricing assumptions

[bookmark: _Toc242091102]How goods and services are priced and assessed for payment
Clause 11 in NEC3 Supply Contract, (SC3) core clauses states:

	Identified and defined terms
	11
11.2
	
(11) The Prices are the amounts stated in the price column of the Price Schedule.  Where a quantity is stated for an item in the Price Schedule, the Price is calculated by multiplying the quantity by the rate.


	
	
	(12) The Price Schedule is the price schedule unless later changed in accordance with this contract.


	Assessing the amount due
	50.2
	The amount due is

the Price for each lump sum item in the Price Schedule which the Supplier has completed, 
where a quantity is stated for an item in the Price Schedule, an amount calculated by multiplying the quantity which the Supplier has completed by the rate,
plus other amounts to be paid to the Supplier,
less amounts to be paid by or retained from the Supplier.

Any tax which the law requires the Purchaser to pay to the Supplier is included in the amount due.




This confirms that the Supply Contract is a priced contract where the Prices are derived from a list of items of goods and services which can be priced as lump sums or as expected quantities of goods and services multiplied by a rate, or a mix of both.
[bookmark: _Toc242091103]Function of the Price Schedule
Clause 53.1 states: “Information in the Price Schedule is not Goods Information”.  This confirms that instructions to do work or how it is to be done are not included in the Price Schedule but in the Goods Information.  This is further confirmed by Clause 20.1 which states, “The Supplier Provides the Goods and Services in accordance with the Goods Information”. Hence the Supplier does not Provide the Goods and Services in accordance with the Price Schedule.   The Price Schedule is only a pricing document.  
[bookmark: _Toc242091104]Preparing the price schedule
Items in the price schedule may have been inserted by the Purchaser and the tendering supplier should insert any additional items which he considers necessary.  Whichever party provides the items in the price schedule the total of the Prices is assumed to be fully inclusive of everything necessary to Provide the Goods and Services as described at the time of entering into this contract.

It will be assumed that the tendering supplier has 

· Read Pages 8, 11, 12 and Appendix 5 of the SC3 Guidance Notes before preparing the price schedule;
· Included in his Prices and rates for correction of Defects (core clause 43.1) as there is no compensation event for this unless the Defect is due to a Supplier’s risk;
· Spread the cost of doing work he chooses not to list as separate items in the price schedule across other Prices and rates in order to fulfil the obligation to Provide the Goods and Services for the tendered total of the Prices; 
· Understood that there is no adjustment to lump sum prices in the price schedule if the amount, or quantity, of work within that lump sum item later turns out to be different to that which the Supplier estimated at time of tender. The only basis for a change to the Prices is as a result of a compensation event per clause 60.1;
· Understood that the Supplier does not have to allow in his Prices and rates for matters that may arise as a result of a compensation event.

[bookmark: _Toc242091105]Format of the price schedule
Entries in the first four columns in the price schedule in section C2.2 are made either by the Purchaser or the tendering supplier. 

If the Supplier is to be paid an amount for the item which is not adjusted if the quantity of work in the item changes, the tendering supplier enters the amount in the Price column only, the Unit, Quantity and Rate columns being left blank.

If the Supplier is to be paid an amount for the item which is the rate for the item multiplied by the quantity completed, the tendering Supplier enters the rate which is then multiplied by the Quantity to produce the Price, which is also entered.

If the Supplier is to be paid an amount for an item proportional to the length of time for which the goods and services are provided, a unit of time is stated in the Unit column and the length of time (as a quantity of the stated units of time) is stated in the Quantity column.
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C2.2 the price schedule

Part 1

1. VARIOUS CLASSES OF NEW TRUCKS

	Item
	Description
	Qty
	UOM
	Rate

	1
	TRUCK: T4 LIGHT;4 X 4;>4500 <=7000 KG
	0
	EA
	

	2
	TRUCK: T5AS MEDIUM;4 X 4;>13000 <16000 KG
	0
	EA
	

	3
	TRUCK: T5BD MEDIUM;4 X 4;>16000 <19000 KG
	0
	EA
	

	4
	TRUCK: T11 HEAVY;6 X 6;26000 KG
	0
	EA
	

	5
	TRUCK: T5AD MEDIUM;4 X 4;>13000 <16000 KG
	0
	EA
	

	6
	LICENSING AND REGISTRATION
	0
	LE
	

	7
	HANDLING FEE
	0
	LE
	

	8
	DELIVERY CHARGE
	0
	LE
	

	9
	TOWBAR MOTOR VEH: PIN
	0
	EA
	

	10
	REFLECTOR SET WRNG TRIANGLR: PLASTIC;RED
	0
	EA
	

	11
	SENSOR: PARK DISTANCE CONTROL ASSISTS;12
	0
	EA
	

	12
	HEAVY-DUTY SINGLE-CAB 4x4 LIGHT DELIVERY VEHICLES
	0
	EA
	




Part 2

1. NEW HEAVY-DUTY SINGLE-CAB 4X4 LIGHT DELIVERY VEHICLES


	Item
	Description
	Qty
	UOM
	Rate

	1
	VEHICLE CMMRCL:LDV;L9D;DIESEL;4X4;LWB                                  
	0
	EA
	

	2
	TOWBAR MOTOR VEH:PIN                                                                           
	0
	EA
	

	3
	REFLECTOR SET WRNG TRIANGLR :PLASTIC;RED                             
	0
	EA
	

	4
	SENSOR:PARK DISTANCE CONTROL ASSISTS;12                              
	0
	EA
	

	5
	LICENSING AND     REGISTRATION                                                           
	0
	EA
	

	6
	HANDLING     FEE                                                                                             
	0
	LE
	

	7
	DELIVERY      FEE                                                                                               
	0
	LE
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[bookmark: _Toc85847724][bookmark: _Toc86542135][bookmark: _Toc88827034][bookmark: _Toc103393483][bookmark: _Toc103395045][bookmark: _Toc103400607][bookmark: _Toc106546957][bookmark: _Toc106547721][bookmark: _Toc106547927][bookmark: _Toc107068460][bookmark: _Toc107118689][bookmark: _Toc107119174][bookmark: _Toc107119609][bookmark: _Toc107120915][bookmark: _Toc107192869][bookmark: _Toc107193261][bookmark: _Toc107193444][bookmark: _Toc107193690][bookmark: _Toc107193834][bookmark: _Toc107194041][bookmark: _Toc107194486][bookmark: _Toc107201199][bookmark: _Toc137798036][bookmark: _Toc229128239][bookmark: _Toc232940110][bookmark: _Toc242091106]Part 3: Scope of Work









	Document reference
	Title
	No of pages

	
	This cover page
	1

	C3.1
	Purchaser’s Goods Information
	8

	C3.2
	Supplier’s Goods Information
(insert at award stage or delete if not applicable)
	1

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	Total number of pages
	10
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[bookmark: _Toc107192870][bookmark: _Toc107193262][bookmark: _Toc107193445][bookmark: _Toc107193691][bookmark: _Toc107193835][bookmark: _Toc107194042][bookmark: _Toc107194487][bookmark: _Toc107201200][bookmark: _Toc137798037][bookmark: _Toc229128240][bookmark: _Toc232940111][bookmark: _Toc242091107]C3.1: Purchaser’s Goods Information


Part 3: Scope of Work	29
C3.1: Purchaser’s Goods Information	30
Overview and purpose of the goods and services	31
Specification and description of the goods	31
Purchaser’s design	31
Procedure for submission and acceptance of Supplier’s design	31
Other requirements of the Supplier’s design	31
Use of Supplier’s design	32
Manufacture & fabrication	32
Factory acceptance testing (FAT)	32
Other tests and inspections and commissioning in place of use	32
Operating manuals and maintenance schedules	32
Supply Requirements	33
Specification of the services to be provided	33
Constraints on how the Supplier Provides the Goods	33
Programming constraints	33
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[bookmark: _Toc137798038][bookmark: _Toc229128241][bookmark: _Toc232940112][bookmark: _Toc242091108]Overview and purpose of the goods and services
Eskom SOC Ltd, Distribution Gauteng Cluster, requires Supply & delivery of various classes of new trucks & new heavy-duty single-cab 4x4 Light Delivery Vehicles on “an as & when” required basis for the period of 3 years at Gauteng Cluster . The trucks will support the operational and maintenance requirements of the Distribution Gauteng Cluster and will operate across various Maintenance and Operations sites and Support Functions.

Eskom requires heavy-duty single-cab 4x4 LDVs to support field activities in rural areas, construction and maintenance sites, distribution network servitudes, gravel roads, agricultural and mining environments, remote locations and emergency-response operations. Vehicles may be used for transporting employees, tools and equipment under variable road and weather conditions.

The Supplier shall be responsible for the supply, delivery, licensing and handover of the required trucks in accordance with the specifications and requirements stated in the Contract and the applicable Purchase Order. Each truck shall be delivered in perfect working order, compliant with applicable statutory and roadworthiness requirements, and ready for immediate use on public and rural roads.

The trucks shall be suitable for their intended operational requirements and capable of safe, reliable and efficient operation under South African road, operating and weather conditions.

The Supplier's services shall include all activities necessary for the successful delivery and handover of the trucks, including, where applicable, licensing, registration, delivery to the specified location, provision of relevant documentation and handover of the vehicles in an operational condition. The specific class, quantity, requirements, delivery location and Delivery Date shall be stated in the applicable Purchase Order.
[bookmark: _Toc242091109]Specification and description of the goods
The following list of specifications are applied to this contract.

	Item No
	Document Title

	1
	Specification



	2
	SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES





[bookmark: _Toc137798056][bookmark: _Toc229128259][bookmark: _Toc232940131][bookmark: _Toc242091110]Purchaser’s design
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Other requirements of the Purchaser’s design – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc137798058][bookmark: _Toc229128261][bookmark: _Toc232940133][bookmark: _Toc242091111]Procedure for submission and acceptance of Supplier’s design
The following list of specifications are applied to this contract.

	No.
	Unique Identifier
	Revision
	Document Title

	1
	
	
	Specification




	1
	
	
	SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES





[bookmark: _Toc137798059][bookmark: _Toc229128262][bookmark: _Toc232940134][bookmark: _Toc242091112]Other requirements of the Supplier’s design
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Other requirements of the Supplier’s design – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc137798060][bookmark: _Toc229128263][bookmark: _Toc232940135][bookmark: _Toc242091113]Use of Supplier’s design
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Use of Supplier’s design – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc242091114]Manufacture & fabrication
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Manufacture and fabrication – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc242091115]Factory acceptance testing (FAT)
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Factory Acceptance Testing (FAT) – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc242091116]Other tests and inspections and commissioning in place of use
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Other tests and inspections and commissioning in place of use – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc137798063][bookmark: _Toc229128266][bookmark: _Toc232940138][bookmark: _Toc242091117]Operating manuals and maintenance schedules
Refer to the list of specifications attached on 2 Specification and description of the goods. Any other specification or requirement not listed under section 2 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order. The Supplier shall comply with the requirements contained in the Invitation to Tender (ITT) and the Purchaser’s Goods Information in relation to the following: Operating manuals and maintenance schedules – as specified in the applicable section of the Purchaser’s Goods Information.

[bookmark: _Toc242091118]Supply Requirements
The Supply Requirements for this contract are in an Annexure A to the Contract Data provided by the Purchaser. 

[bookmark: _Toc242091119]Specification of the services to be provided
Refer to the applicable technical specifications and requirements attached under Item 1 of the Purchaser’s Goods Information.

Any other specification or requirement not listed under Item 1 will be provided by the Supplier and agreed with the Supply Manager prior to the conclusion of a Purchase Order.


[bookmark: _Toc242091120]Constraints on how the Supplier Provides the Goods
[bookmark: _Toc137798048][bookmark: _Toc229128251][bookmark: _Toc232940122][bookmark: _Toc242091121]Programming constraints 
The Supplier’s delivery programme, including the required delivery dates and lead times, shall be discussed and agreed with the Supply Manager prior to the conclusion of each Purchase Order.


[bookmark: _Toc242091122]Work to be done by the Delivery Date
The Supplier shall ensure that the required trucks are fully supplied, compliant with the specified requirements, and ready for delivery by the Delivery Date stated in the Purchase Order. Specific requirements shall be discussed and agreed with the Supply Manager prior to the conclusion of each Purchase Order.

[bookmark: _Toc242091123][bookmark: _Toc137798079][bookmark: _Toc229128283][bookmark: _Toc232940155]Marking the goods 
General requirements for the marking and identification of the goods, including Eskom identification or branding where applicable, shall be discussed and agreed with the Supply Manager prior to the conclusion of each Purchase Order.


[bookmark: _Toc242091124]Constraints at the delivery place and place of use
All deliveries must take place during Eskom working hours, supplier to obtain permits and submit all necessary documents in terms of security. Supplier to familiarize themselves with delivery place and ensure access is possible in terms of road conditions, height restrictions etc.  


[bookmark: _Toc137798090][bookmark: _Toc229128293][bookmark: _Toc232940165][bookmark: _Toc242091125]Cooperating with Others
The Supplier’s delivery personnel will have to comply to all security and safety requirements prior to the entry at the place of delivery.


[bookmark: _Toc242091126]Services & other things to be provided by the Purchaser or Supplier
Service plans and all other services to be provided by the purchaser or the supplier will be agreed with the Supply manager prior to conclusion of the purchase order.



[bookmark: _Toc137798043][bookmark: _Toc229128246][bookmark: _Toc232940117][bookmark: _Toc242091127]Management meetings

Regular meetings of a general nature may be convened and chaired by the Supply Manager as follows:

	Title and purpose
	Approximate time & interval
	Location
	Attendance by:

	Risk register and compensation events
	As and when required
	Specified by the supplier manager/MS Teams
	Purchaser, Supplier, and key stakeholders

	Overall contract progress and feedback
	As and when required
	TBC
	Purchaser, Supplier, and key stakeholders



Meetings of a specialist nature may be convened as specified elsewhere in this Goods Information or if not so specified by persons and at times and locations to suit the Parties, the nature and the progress of the manufacture of the goods.  Records of these meetings shall be submitted to the Supply Manager by the person convening the meeting within five days of the meeting.  

All meetings shall be recorded using minutes or a register prepared and circulated by the person who convened the meeting.   Such minutes or register shall not be used for the purpose of confirming actions or instructions under the contract as these shall be done separately by the person identified in the conditions of contract to carry out such actions or instructions.  

[bookmark: _Toc137798044][bookmark: _Toc229128247][bookmark: _Toc232940118][bookmark: _Toc242091128]Documentation control
The contract document and tenders shall be stored in the cabinets at procurement Department. Contractual communication will be in a form of properly compiled letters or forms in a chronological order, attached to emails.

[bookmark: _Ref134768869][bookmark: _Toc137798045][bookmark: _Toc229128248][bookmark: _Toc232940119][bookmark: _Toc242091129]Health and safety risk management
[bookmark: _Toc137798046][bookmark: _Toc229128249][bookmark: _Toc232940120]The Supplier shall comply with the health and safety requirements contained in the Invitation to Tender (ITT) to this Enquiry.
[bookmark: _Toc242091130]Environmental constraints and management
The Supplier shall comply with the environmental criteria and constraints contained in the Invitation to Tender (ITT) to this Enquiry.

[bookmark: _Toc137798047][bookmark: _Toc229128250][bookmark: _Toc232940121][bookmark: _Toc242091131]Quality
The Supplier shall comply with the environmental criteria and constraints contained in the Invitation to Tender (ITT) to this Enquiry.
[bookmark: _Toc232940124][bookmark: _Toc242091132]Invoicing and payment
Within one week of receiving a payment certificate from the Supply Manager in terms of core clause 51.1, the Supplier provides the Purchaser with a tax invoice showing the amount due for payment equal to that stated in the Supply Manager’s certificate.  

The Supplier shall address the tax invoice to Purchaser and include on each invoice the following information:

Name and address of the Supplier and the Supply Manager; 
The contract number and title;
Supplier’s VAT registration number;
The Purchaser’s VAT registration number.
Description of goods and services provided for each item invoiced based on the Price Schedule;
Total amount invoiced excluding VAT, the VAT and the invoiced amount including VAT;


Procedures for invoice submission and payment (e. g. electronic payment instructions)

	General Information
	X

	-	No Pro-forma Invoice
	

	-	Check Vendor number against the Address and name on Tax invoice
	

	-	Insert the Vendor number on Tax invoice (Top right-hand corner)
	

	-	Bank details must be on the invoice or on a attach sheet, but it does not require a bank stamp just a letter)
	

	- Check banking details on invoice against SAP system. If more than one banking account check bank account against banking details on invoice. If banking details not on invoice, write the bank code next to the vendor account (bank code 0002)
	

	- Check Vendor VAT number against the vendor master. (FK03) If VAT number not on master records, prepare a list and forward to Vendor Management to check and update the vendor master records
	

	-	No fax copies of Tax invoices allowed
	

	- No copies of Tax invoices allowed unless originally printed by the Vendor if a photocopy tax invoice, it must be an original “certified copy” (i.e. not a copy of a “certified copy” invoice) from the vendor and check in system if not previously be paid. Put stamp “not previously paid” on invoice
and sign.
	

	-	Ensure that date received stamp is clear on invoice
	

	-	Stamp all Invoices with the Vat stamp, complete and sign (only when VAT is applicable)
	

	-	The stamp should not be stamped over any written information
	

	-	When scanning invoice, check the quality before linking in SAP (inboxes)
	

	
	

	With Reference Invoices
	X

	-	Goods receipt must be done (payment with reference)
	

	-	Ensure that the SAP purchase order number is clear and correct on the invoice
	

	-	GR number to be written on the Invoices
	

	-	If multiple lines on invoice write the line number of the order against the line to ensure that the processors match the correct lines (to ensure that 191100 is matched correctly)
	




[bookmark: _Toc137798051][bookmark: _Toc229128254][bookmark: _Toc232940125][bookmark: _Toc242091133]Insurance provided by the Purchaser
The Purchaser only provides insurance should the goods be provided ex-works from the point of collection. The Supplier is to provide all insurances up to the point of delivery where they are responsible to deliver.

[bookmark: _Toc137798052][bookmark: _Toc229128255][bookmark: _Toc232940126][bookmark: _Toc242091134]Contract change management 
There are no additional requirements to those stipulated in Core Clause 6.


[bookmark: _Toc137798053][bookmark: _Toc229128256][bookmark: _Toc232940127][bookmark: _Toc242091135]Provision of bonds and guarantees
The form in which a bond or guarantee required by the conditions of contract (if any) is to be provided by the Supplier is given in Part 1 Agreements and Contract Data, document C1.3, Sureties.  

The Purchaser may withhold payment of amounts due to the Supplier until the bond or guarantee required in terms of this contract has been received and accepted by the person notified to the Supplier by the Supply Manager to receive and accept such bond or guarantee.  Such withholding of payment due to the Supplier does not affect the Purchaser’s right to termination stated in this contract. 

[bookmark: _Toc137798054][bookmark: _Toc229128257][bookmark: _Toc232940128][bookmark: _Toc242091136]Records of Defined Cost, payments & assessments of compensation events to be kept by the Supplier
All records of defined costs are to be filed and access granted to the Supply Manager at any time upon request.

[bookmark: _Toc137798064][bookmark: _Toc229128267][bookmark: _Toc232940139][bookmark: _Toc242091137]Procurement
[bookmark: _Toc137798068][bookmark: _Toc229128272][bookmark: _Toc232940144][bookmark: _Toc242091138]Subcontracting
[bookmark: _Toc137798069][bookmark: _Toc229128273][bookmark: _Toc232940145][bookmark: _Toc242091139]Preferred subcontractors
Refer to the attachments contained in the ITT to this enquiry.

[bookmark: _Toc137798071][bookmark: _Toc229128275][bookmark: _Toc232940147][bookmark: _Toc242091140]Limitations on subcontracting
Refer to the attachments contained in the ITT to this enquiry.


[bookmark: _Toc137798077][bookmark: _Toc229128281][bookmark: _Toc232940153][bookmark: _Toc242091141]Spares and consumables
Not Applicable


[bookmark: _Toc242091142]Other requirements related to procurement
Refer to the attachments contained in the ITT to this enquiry.

[bookmark: _Toc242091143]Cataloguing requirements by the Supplier
Not Applicable
[bookmark: _Toc137798122][bookmark: _Toc229128325][bookmark: _Toc232940197][bookmark: _Toc242091144]List of drawings
[bookmark: _Toc137798123][bookmark: _Toc229128326][bookmark: _Toc232940198][bookmark: _Toc242091145]Drawings issued by the Purchaser
This is the list of drawings issued by the Purchaser at or before the Contract Date and which apply to this contract.  


	Drawing number
	Revision
	Title

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



[bookmark: _Toc137798124][bookmark: _Toc229128327][bookmark: _Toc232940199][bookmark: _Toc242091146]C3.2	Supplier’s Goods Information

	This section of the Goods Information will always be contract specific depending on the nature of the goods and services.
It is most likely to be required for supply contracts where the tendering supplier will have proposed specifications and schedules for the goods and services, which once accepted by the Purchaser prior to award of contract now become obligations of the Supplier per core clause 20.1.





This section could also be compiled as a separate file.
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To whom it may concern 
 	 	 	 
This letter serves to confirm the insurance cover as follows: 
 
 
Insurer 	 	 	 	: 	ESCAP SOC Ltd 
 
Insured 	 	 	 	:  	Eskom SOC Ltd including National Transmission  
Company of South Africa (NTCSA) SOC Ltd, Eskom  Rotek Industries SOC Ltd, and other its wholly owned  subsidiaries 
 
Additional Insureds                            :           Entities dictated by financial or operational interest of                                                                                the Insured, each for their respective rights and interest  
All contractors undertaking work for or on behalf of the Named Insured but only in respect of the execution of any contract(s) (the “Contracts”) between the contractor and Named Insured (it being understood that where the Named Insured undertakes the work they shall be deemed to be the “Contractor” provided that their rights hereunder shall not exceed the rights of any independent contractor working on behalf of the Named Insured) (hereinafter called the “Contractor”). 
 
All subcontractors employed by the Contractor and all other subcontractors (whether nominated or otherwise engaged but only in respect of the fulfilment of the contract(s)) (hereinafter called the "Subcontractor") for their respective rights and interests. 
 
Any reference to Insured in this Policy shall apply to the 
Named Insured and where applicable the Additional Insured listed above. Cover in respect of contractors and subcontractors shall only be provided to the extent that the Named Insured undertakes in the contracts with the 
 ESCAP SOC Ltd 
Maxwell Drive Megawatt Park Sunninghill Sandton 
PO Box 1091 Johannesburg 2000 SA     
Tel +27 11 800 6804 Fax +27 11 800 4737  www.eskom.co.za 
    Escap SOC Ltd  Reg No 1993/003340/30 	 
 
 
 
Additional Insured between the Named Insured and 
Contractor and/or Subcontractor to provide the 
 
Insurance coverage found in this policy (hereinafter called the “Insurance Cover”) for such parties 
 
Policy name  	 	 	:  	Annual Construction All Risks  
 
Period of insurance  	 	:  	01 April 2026 – 31 March 2027 
 
Policy limit 	: 	Section I - Contract Works: 
Basic project value of R 500 million up to R 1 billion and 60 months at inception, thereafter unlimited in value and project time up to completion. 
 
Section II - Contract Works Public Liability: 
R25 million, any occurrence or series of occurrences  arising out of one event  
 	 	 	 	 	 	 
Policy coverage 	 	 	: 	Direct physical loss of or damage to any part of the  
Works and property insured including while in transit or at storage, including third party liability. 
 
 	 
Policy deductibles 	 	 	: 	As per table below 
	Deductible 
	Division / Coverage 

	Section I – Contract Works 

	R 500,000 
	Physical Damage to Property 

	R10 000 000 
	Transmission – Theft and Vandalism 

	R 5,000,000 
	Distribution - Theft & Vandalism 

	R1 000 000 
	Eskom Rotek Industries – Theft and Vandalism 

	R 50,000 
	Debris Removal 

	R 50,000 
	Debris Removal (No Damage) 

	R 25,000 
	Borrowing of plant for commission purposes 

	R 1,000 
	Documentation 

	Section II – Contractors’ Public Liability 

	R 50,000 
	Damage resulting from Fire and Spread of Fire 

	R 20,000 
	All other losses 


 
 
 
 	Escap SOC Ltd  Reg No 1993/003340/30 
 
 
Note: 
Cover is only limited to projects declared for the insurance period stipulated above and as verified and finalised by the Insurer. 
 
Please refer your queries to your contact person at Eskom 
 	 
 
 
Yours sincerely 
 
[image: ]________________________ 
Shadrack Sivhugwana 
Escap SOC Ltd – Chief Executive Officer  Date: 04 June 2026  Escap SOC Ltd  Reg No 1993/003340/30 
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1. INTRODUCTION

Eskom SOC LTD Distribution Gauteng Cluster requires supply of 42 Trucks. These trucks operate
across all Distribution Gauteng Cluster. The vehicles are stationed at various Maintenance and
Operations sites & Support Functions.

2. DEFINITIONS AND TERMINOLOGY

Definition

Explanation

Ancillary equipment

Any item purchased and fitted to a vehicle, which is not fitted as
original equipment by the vehicle manufacturer

Accessory equipment

Accessory equipment are "add-ons" a carrier can install on the
vehicle to improve efficiency, safety, comfort, or ease of operation.

Under-run protection
devices

Side under-run protection devices or "lateral protection devices"
occupy larger spaces between axles on a rigid truck or a semitrailer.
They are barriers or plates that sit in the space between axles.
They are designed for the following purposes:
1. To stop other road users such as other vehicles, cyclists, and
pedestrians getting under the rear wheels of a truck or trailer.
2. To minimise the potential damage a roadside obstacle might
cause if the truck turns in too early.

Heavy vehicle (trucks
or yellow plant)

A vehicle with a gross vehicle mass of more than 3 500 kg.

Heavy axle" means an axle whose wheels are fitted with tyres of a
size (bead seat diameter) greater than 406.4 mm (16 inches), or an
axle with more than two wheels regardless of tyre size, but excluding
any axle of a motorcycle, a motor tricycle, or a motor car.

'Heavy vehicle" means a motor vehicle with at least one heavy

axle and/or any vehicle that has been principally designed or

adapted for the convenience of persons exceeding 16 in number.






3. ABBREVIATION

Abbreviation Explanation
LDV Light delivery vehicle

NRTA National road traffic act

SRS Supplemental restraint system

LWB Low Wheelbase

SWB Short Wheelbase

HGC High ground clearance

ABS Antl-Lock braking system

BEV Battery electric vehicle

EV Electric vehicle

BU Business unit

GVM Gross vehicle mass

ISO International organization for standardization
LDV Light delivery vehicle

LWB Long wheelbase

NRTA National road traffic act

OBD/II Onboard diagnostic second-generation
RTM Act Road traffic management act.

VMD Vehicle-monitoring device

A&F Assurance and forensic department
RMI Retail motor industry

SANS South African national standards

4. APPLICABLE LAWS AND LEGISLATIONS

[1] SANS 1563 — The strength of large passenger vehicle superstructures (Rollover protection)

[2] 1SO 9001 Quality management systems

[3] ISO 45001 Occupational health and safety






[4] National Road Traffic Act 93 of 1996
[5] National Environmental Management: Air Quality Act No 39 of 2004

5. SCOPE OF WORK

The supply and delivery of various class of trucks to Distribution Gauteng Cluster on a as and
when required basis for period of 3 years. The bid is for the supply, delivery, licensed, fuelled
and hand over of the fleet in perfect working order and ready for immediate use on public and
rural roads. The vehicles shall be designed for and be capable of efficient and safe operation
under all South African weather conditions.

5.1 VEHICLE CATEGORIES

TAAD Light Truck 4x4 GVM (Dual wheel application)

T5AD Medium Truck 4x4 > 13000 <16000 GVM (Dual wheel application)
T5AS Medium Truck 4x4 >13000 <16000 GVM (Single wheel application)
T5BD Medium Truck 4x4 > 16000 < 19000GVM (Dual wheel application)
Til Heavy Truck 6x6 26000 GCM (Single Wheel application)

Eskom reserves the right to order vehicles on an as-and-when required basis during the contract
period. By virtue of being appointed as one of the successful suppliers does not entitle the
supplier to impose the placing of orders to the full value at any given time during the contract

period.

6. TECHNICAL SPECIFICATION/DETAILED SCOPE OF WORK

6.1 STANDARD REQUIREMENTS

All commercial vehicles shall comply with the provisions of the National Road
Traffic Act, as amended

Vehicle tools required to be supplied with the vehicle shall consist of at least a
suitable jack handle, wheel nut spanner and 2x emergency warning signs triangle
and/or cones).

A spare wheel must be supplied with the provision to permanently mount the
spare

All vehicles must be supplied with front and rear backing plates for the fitment of
number plates.

All vehicles that require Road Worthy Certificates should be supplied with mass
plates affixed to the vehicle.





All vehicles that require Road Worthy Certificates should be supplied with all
accessories, fitment and signage as required (e.g. fire extinguisher, seating

capacity, speed limitation sign and conspicuity tape)

The following categories of vehicles must be supplied standard as a minimum, as
provided below: Commercial vehicle specifications - gross vehicle mass (GVM) 3
500 kg and above (including heavy commercial vehicles with GVM above 16 000

kg and abnormal vehicles):

LR NOURWNE

18.

19.

20.

21.

22.

Radio/ MP3 player/blue tooth
Central locking system

Power steering

Fog lights

Immobiliser

Alarm

Air Conditioner
Driver and passenger airbags.

ABS braking system.

Daytime running lights

Seat Belts: SABS approved

Factory-fitted power steering

Reverse lights

Reverse alarm / beeper

Driver and passenger seatbelt reminder/alarm

Head light on reminder indicator/alarm when vehicle is
switch off

All seats are to be covered with a durable fabric and fitted

with headrests

Yellow reflective tape that must be fitted in accordance with the
National Road Traffic Act specification xix. Anti-spray mudflaps xx.
Under-run protection device in accordance with the SANS 1055
standards

Chevron warning plates in accordance with the National Road
Traffic Act specification xxii. A speed limit warning sign in
accordance with the National Road Traffic Act specification.

Any other apparatus (including large toolboxes) shall be fitted in
such a manner that it would be sufficiently secured in the event
of vehicle rollover or collision and would not create a risk by
weakening the structure of the vehicle.

Applicable warning signs for the type of transportation should be

fitted in accordance with legislation.

Homologation of load body according to (Road traffic Act and

Regulations No. 192A)





23.  Allowances must be made on the load body sizes of relevant LDV's
and trucks for additional fitments to the trucks such as cranes,
hydraulic platforms (cherry pickers), etc. to ensure that the fitment
of the accessories and the load body of the fleet item is compatible
with the chassis of the fleet item

6.2 TABLE OF VEHICLE CATEGORIES

Category Description Code

Truck 4x4 FIC
Light Truck 4x4 D 4x4 >4500 < 7000 kg D/Wheel TA4AD
Medium Truck 4x4 >13000 < 16000 kg, GVM D/Wheel T5AD
Medium Truck 4x4 >13000 < 16000 kg, GVM S/Wheel T5AS
Medium Truck 4x4 > 16000 < 19000 kg, GVM D/Wheel T5BD

Extra heavy Truck 6x6
Extra Heavy Truck 6x6 > 26000 kg, GVM & above Til

Category "T4AD" Light Truck 4x4 > 4500 < 7000 kq (Dual wheel application)

Vehicle Job Required for carrying goods, equipment and passengers up to a GVM of|
Description | 7000 kg on all types of road surfaces with up to 80 % off road usage.

(Licence code Cl)






Technical
Specification

kW output: Minimum 100 kW
Nm torque: Minimum 350 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating "2600 kg to 2800kg"
Permissible rear axle rating "4300 kg 6000kg"
DIT rating: " max 7000 kg"
Wheelbase: "3365 mm to 4000 mm
Air conditioner factory fitted
Driver and passenger airbags
Driver and passenger seatbelt reminder indicator / alarm
Daytime run lights
ABS brakes
Power steering
Radio/ MP3 player/blue tooth
Two emergency triangles
Rear overhang: Not to exceed 50 % of wheelbase
Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system
Trailer brake control (optional)
Fitted towing/recovery facility on front
Tyre (Size), As per manufacture 7.50R16-10 PR (up to 80% off road
_usage) Compatible diff-ratio.
Noise Level: Not to exceed 75db
Colour: White
Reverse alarm / beeper

Permitted
accessory’s

Truck mounted crane, 6 Ton metre range
Tail lift 1.5 Ton capacity
1 1m round to bottom of basket aerial platform Live line SSI






Permitted
ancillaries are
optional

Tow bar

Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's
gearbox is engaged (or hand-brake failsafe system / alarm) (in any
gear).

Flatbed drop side

Cargo van body

Tool cab

Ladder rack

"H" frame

Toolboxes

Stainless steel water tank

Working lights

Amber revolving light

Under run bumper fixed or energy absorbing type

Wheel Flaps: SABS 1496 specification

Yellow reflective tape that must be fitted (Road traffic act and
regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations No. 192A)

Medium Truck 4x4 > 13000 < 16000 kq GVM

Category "T5AS" Single rear tyres (Single - 12R 20 Tyres)

Vehicle Job |Required for carrying goods, equipment, and passengers up to a GVM of
Description 116000 kg on all types of road surfaces with up to 80 % off road usage.






Technical
Specification

kW output: Minimum 170 kW

Nm torque: Minimum 750 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating "4700kg to 5500kg"
Permissible rear axle rating "max 8000 kg" single rear wheels
D/T rating: "17500 to 21000kg"

Wheelbase: "3900mm to 4800mm"

Air conditioner factory fitted

Driver and passenger airbags

Dat time running light

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Rear overhang: Not to exceed 50 % of wheelbase
Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system
Trailer brake control (optional)

Fitted towing/recovery facility on front

Tyres: As per manufactures specifications (Single rear tyres - 12R 20)
Noise Level: not to exceed 75db

Reverse alarm / beeper

Permitted
accessory’s

Truck mounted crane, 13 Ton metre range
Tail lift 2-Ton capacity
15m round to bottom of basket aerial platform Live line SSI






Permitted ow bar
ancillaries are Air conditioner
optional Hour meter
Interlock hand brake system
PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's gearbox
is engaged (or hand-brake failsafe system / alarm) (in any gear). Flatbed
drop side cargo van body
Tool Cab
Ladder rack frame
Toolboxes
Stainless steel water tank
Working lights
Amber revolving light
Under run bumper fixed or energy absorbing type
Wheel Fla s: SABS 1496 specification
Boor Machine
Air charge line to front and rear & coupling

Yellow reflective tape that must be fitted. (Road traffic Act and Regulations
No. 192A)

Homologation of load body according to (Road traffic Act and Regulations
No. 192A
Medium Truck 4x4 > 13000 < 16000 kq GVM

Category "T5AD" (Dual rear tyres)

Vehicle Job Required for carrying Goods, equipment, and passengers up to a GVM of
Description 16000 kg on all types of road surfaces with up to 80 % off road usage,






Technical
Specification

KW output: Minimum 170kw

Torque: Minimum 706Nm to 810Nm

Diesel Powered (Normally aspirated or Turbo)
Permissible Front axle Rating "4700kg to 5500kg 'i
Permissible Rear axle Rating "max 8000 kg" single rear wheels
D/T Rating: "17500 to 21000kg"

Wheelbase: "3900mm to 4800mm"

Air Conditioner Factory fitted

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Two emergency triangles

Rear Overhang: Not to exceed 50 % of wheelbase
Manufactures approved Engine Protection Device
Chassis to facilitate the fitting of hydraulic crane

Fully Synchromesh Gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system

Trailer brake control (optional)

Fitted towing/recovery facility on front

Tyres: As per Manufactures Specifications (Single rear tyres - 12R 20)

Noise Level: not to exceed 75db
Reverse alarm / bee

Permitted
accessory's

Truck Mounted Crane, 13 Ton Metre range
Tail lift 2-ton capacity
15m round to bottom of basket Aerial platform Live line SSI






Permitted
ancillaries are
optional

Tow bar

Air conditioner

Hour meter

Interlock hand brake system

PTO

Flat Bed Drop side

Cargo van body

Tool cab

Ladder Rack

H" Frame

Toolboxes

Stainless steel Water Tank

Working Lights

Amber Revolving Light

Under run bumper fixed or energy absorbing type
Wheel Flaps: SABS 1496 specification Boor Machine
Air charge line to front and rear & coupling.

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations

No. 192A

Medium Truck 4x4 > 16000 < 19000 kg GVM

Category "T5BD" Dual rear tyres -T5BD

Vehicle Job
Description

Required for carrying goods, equipment and passengers up to a GVM of
19000 kg. On all types of road surfaces with up to 80 % off road usage.






Technical
Specification

kW output: Minimum 170 kW Nm
torque: Minimum 810 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating 17100kg to 7700kg"
Permissible rear axle rating "9000 kg"

D/T rating: " 28000 kg"

Wheelbase: "Minimum 4500 mm and 4800 maximum"
Rear overhang: Not to exceed 50 % of wheelbase

Air conditioner factory fitted

Day time running light

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Chassis to facilitate the fitting of hydraulic crane front or rear mounted
Fully synchromesh gearbox with manual shift /automatic gearbox.
Gear ratio: Top gear 1 :1 and Lowest gear higher than 8:1

Top speed of vehicle max 100kmph (determine by gear ratio, no
electronic speed limiters allowed)

Independent transfer box (4x4)

Diff ratios to be determined by top speed of vehicle Trailer brake control
Fitted towing/recovery facility on front

Tyres: As per manufactures specifications Noise Level: not to exceed
75db

Reverse alarm / beeper

Permitted
accessory's

Truck mounted crane, 16 Ton metre range.
HHH / DTH drilling rig (With compressor separately)
15m round to bottom of basket aerial platform Live line OCI






Permitted Tow bar

ancillaries are Air conditioner

optional Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's gearbox
is engaged (or hand-brake failsafe system / alarm) (in any gear). Flatbed
drop side / Cargo van body Ladder rack

“H” frame

Toolboxes

Stainless steel water tank

Working lights

Amber revolving light

Under run bumper fixed or energy absorbing type

Wheel flaps: SABS 1496 specification

Air charge line to front and rear & coupling

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations No. 192A)

Extra Heavy Truck 6x6 > 26000 kq GVM & above

Category "T11 "(Dual rear tyres or Single rear tyres)

Vehicle Job Required for carrying goods & equipment of up to 75000 kg GCM on all types
Description of road surfaces short & long distance. (Licence code ECI)






Technical
Specification

kW output: Minimum 300

kW Nm torque: Minimum

1500 Nm

Diesel powered (Normally aspirated or turbo)

Permissible front axle rating "max 8000 kg'

Permissible rear axle rating "max 16000kg single and 18000kg
dual" D/T rating: "max 56000 kg"

Wheelbase: (Centre front axle to centre of rear axle unit) 4525mm
Air conditioner factory fitted

Daytime running lights

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm

Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh

Brakes to be air assisted or full air dual system
Trailer brake control

Fitted towing/recovery facility on front

5th wheel manufactures approved.

Tyres: As per manufactures specifications (Tredco)
Noise Level: Not to exceed 75db

Reverse alarm / beeper

Permitted
accessory's

Truck mounted crane max 22 Ton metre range
25 M bottom to basket OCI, SSI aerial platform

Permitted
ancillaries are
optional

Air conditioner

Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or
mechanical interlock to disallow the PTO from operating while the
vehicle's gearbox is engaged (or hand-brake failsafe system / alarm)
(in any gear).

Toolboxes

Working lights

Amber revolving light

Wheel flaps: SABS 1496 specification

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No,192A






Fitted towing/recovery facility on front
5" wheel manufactures approved.

Tyres: As per manufactures specifications
(Tredco) Noise Level: Not to exceed 75db
Reverse alarm / bee er

Permitted Truck mounted crane max 22 Ton metre range
accessory’s 25 M bottom to basket OCI, SSI aerial platform
Permitted Air conditioner

Ancillaries Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or
mechanical interlock to disallow the PTO from operating while the
vehicle's gearbox is engaged (or hand-brake failsafe system / alarm)
(in any gear). Toolboxes

Working lights

Amber revolving light

Wheel flaps: SABS 1496 specification

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Re illations No. 192A

6.2 MODEL CHANGE

e Any known model changes/enhancements may be stipulated by bidders in the bid
response and accommodated in the item's price stipulated upfront in the pricing
Schedule. Thus, price changes due to model changes/enhancements will not be
accepted post the award of the contract.

e Should a vehicle model or shape change (or facelift) the new model should either
be offered under the same price as the previous model or as a separate item at the
time of bid submission or resubmission of pricing process.

e When offering it as a separate item, the bidder must indicate the date at which the
model change will become effective as well as the date when the old model will no
longer be available.

e Model changes/enhancements that are offered to Eskom at no additional cost must
remain within the same vehicle category as the original item offered.

6.3 VEHICLE REGISTRATION AND LICENSING

The service provider will be responsible for registration and licensing of the vehicles.





6.4 WARRANTEES/GUARANTEES

e All vehicles supplied in terms of this contract are required to have a
warrantee/guarantee which is to be effective on the date that Eskom take possession
of the vehicle.

e The warrantee/guarantee must be valid in accordance with the manufacturing
standards of the vehicle as stated by the manufacturer.

e Full details of the vehicle warranties/guaranties must be provided electronically and
printed as part of the bid submission.

e The service provider guarantees that the items supplied under the contract are new
and unused.

e The insurance of items against loss or damage incidental to manufacture or
acquisition, transportation, storage and delivery will be the responsibility of the
service provider. Any damaged parts of the vehicle because of manufacture or
acquisition, transportation, storage and delivery must be replaced with new and
unused parts.

Eskom must be informed if the ordered vehicle is damaged while in transit.
Eskom retains the right to take delivery or refuse to take delivery of any vehicle once
it was damaged.

e Eskom will not take possession of any vehicle exceeding 200km on the odometer of
the vehicle at the time of delivery, unless such vehicle needed to be moved for
conversion or the fitment of accessories.

e The successful bidder will be required to provide Eskom with documentation or
certification confirming the warrantee, service plan and maintenance plan.

6.5TRAINING

e Hand-over training or vehicle orientation is required when vehicles are delivered
this will include the training of individuals to operate a specific vehicle and all accessories
thereto safely, economically and effectively.

e Hand-over training will have to be provided for a minimum of two officials as identified by
Eskom at the time of delivery of the vehicle at no additional cost to Eskom.
The service provider can make available pre-arranged group sessions for the
introduction of the new vehicle models.

e Any service provider on the contract will need to train up any individual that is
identified by Eskom for the operation of any vehicle supplied on the contract at
no additional cost.
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SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

® €skom

SCOPE OF WORK

SUPPLY, DELIVERY, REGISTRATION AND SUPPORT OF HEAVY-DUTY SINGLE-CAB 4x4 LIGHT DELIVERY VEHICLES
Brand-neutral, performance-based procurement specification

® E€skom

Do e d D
Business unit Eskom Distribution
Operational area Gauteng Cluster and other Eskom operations, as instructed
Contract basis As and when required
Vehicle class New heavy-duty single-cab 4x4 Light Delivery Vehicles (LDVs)
Prepared by Vuyokazi Maseti
Status Draft for review and approval
Document date 09 September 2026

IMPORTANT

No make, brand, model or country of origin is prescribed. Any compliant vehicle may be offered, provided it meets every mandatory functional,
safety, legal, technical, warranty and support requirement in this Scope of Work.

ABSTRACT

This document defines the requirements for the supply, delivery, licensing, registration, fitment, handover, warranty of new heavy-duty single-
cab 4x4 Light Delivery Vehicles for Eskom operational use for a period of three years. The specification is deliberately brand-neutral and
outcome-based to promote fair competition while ensuring that vehicles are safe, durable, serviceable and suitable for demanding on-road and
off-road conditions.

CONFIGURATION CONTROL

0 09 September 2026 Vuyokazi Maseti Recreated as a brand-neutral 4x4 LDV Scope of Work
Actio ame Designatio gnature Date
Compiled Vuyokazi Maseti Fleet Manager - Gauteng Cluster e 09.09.2026
Reviewed ( N
Sl & b
Approved Xolile Mlaba Senior Manager Gauteng (Acting) \M\(&}‘h 09/09/2026

1. INTRODUCTION

Eskom requires heavy-duty single-cab 4x4 LDVs to support field activities in rural areas, construction and maintenance sites, distribution
network servitudes, gravel roads, agricultural and mining environments, remote locations and emergency-response operations. Vehicles may be
used for transporting employees, tools and equipment under variable road and weather conditions.

The procurement shall not be restricted to a particular manufacturer. The supplier may offer any make and model that is commercially available
in South Africa and that fully satisfies the mandatory requirements and provides adequate national or regional support.

2. PURPOSE AND OBIJECTIVES

The purpose of this Scope of Work is to appoint minimum of one and maximum of four capable suppliers to provide new heavy-duty single-cab
4x4 LDVs on an as-and-when-required basis for a period of three years. The objectives are to:
e obtain fit-for-purpose vehicles through fair, brand-neutral competition;
ensure legal compliance, roadworthiness and occupant safety;
provide dependable off-road mobility, payload and towing capability;
secure predictable warranty, servicing, parts and technical support;
standardise minimum tow-bar installation and documentation without prescribing a proprietary platform;
apply measurable inspection and acceptance criteria at delivery.
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® E€skom

3. DEFINITIONS AND ABBREVIATIONS

SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

A drivetrain capable of supplying driving force to all four wheels, with driver-selectable or automatic four-wheel-

4x4/4WD drive functionality suitable for off-road use.

LDV A Light Delivery Vehicle configured exclusively as a single-cab pickup and specified for heavy-duty
commercial and field operations.

OEM Original Equipment Manufacturer.

Supplier The contracted party responsible for the complete supply, fitment, delivery, documentation and support

obligation.

Mandatory requirement

Arequirement that must be met. A material failure may render an offer technically unacceptable.

GVM

Gross Vehicle Mass stated by the OEM.

GCM Gross Combination Mass stated by the OEM.

Payload Eermissible carrying capacity calculated and declared in accordance with the OEM specification and legal
limits.

PDI Pre-delivery inspection.

SANS South African National Standards.

NRTA National Road Traffic Act 93 of 1996 and applicable regulations.

PDC Park Distance Control

4. APPLICABLE LEGISLATION AND STANDARDS

At the time of delivery, each vehicle and all tow-bar installation shall comply with applicable South African legal and regulatory requirements. The
supplier shall identify the exact standards and approvals applicable to the offered vehicle. These include, where applicable:
National Road Traffic Act 93 of 1996 and regulations;
South African vehicle homologation and certification requirements;
applicable SANS requirements for vehicles, components, glazing, lighting, tyres, towing equipment and electrical tow-bar installation;
Occupational Health and Safety Act 85 of 1993 where work, fitment or handover activities are performed;
National Environmental Management Act 107 of 1998 and applicable emissions requirements;

e OEM manufacturing, body-builder, loading, towing, fitment and warranty instructions.
Where a cited standard is revised, the version legally applicable at the date of manufacture or delivery shall apply, unless Eskom specifies
otherwise in the purchase order.

5. SCOPE OF SUPPLY

The supplier shall provide a complete, operational and road-legal vehicle solution. The scope includes:
sourcing and supplying new, unused 4x4 LDVs;

all specified standard vehicle equipment;

PDI, quality checks and roadworthiness confirmation;

registration, licensing and number plates in the nominated Eskom entity name;

fuel sufficient for handover and operational movement;

delivery to the location stated in each purchase order;

handover documentation, keys, manuals and training;

warranty, service support, parts support and defect rectification.

Quantities, cab configuration, delivery location and optional tow-bar installation will be stated in individual purchase orders. No minimum
volume is guaranteed unless expressly stated in the contract.

6. VEHICLE CATEGORIES

Category

Intended use

Minimum configuration

Category A: Heavy-Duty
Single-Cab 4x4 LDV

Tools, equipment, field maintenance and payload-
focused operations

Two-door single-cab pickup; seating for at least two
occupants; load box.

7. TECHNICAL AND FUNCTIONAL REQUIREMENTS

7.1 Core vehicle requirements

Ref. Requirement Minimum acceptance criterion Bidder evidence
- Factory-new, unused, current production vehicle; not previously registered OEM specification and supplier
T Condition A X - X .
except where required for delivery administration. declaration
Heavy-duty single-cab LDV/pickup with a separate load box and
T2 Body type . . . Brochure/data sheet
commercial-duty chassis construction.
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SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

Ref. Requirement Minimum acceptance criterion Bidder evidence
Functional 4x4/4WD system suitable for low-traction and off-road conditions.
T3 Drivetrain Where low range is not fitted, bidder shall demonstrate equivalent off-road OEM technical data
capability.
) Dlesel.preferred-. Alterna?lveApowertram may pe offered only if range, Technical schedule and
T4 Engine refuelling/charging practicality, payload, towing, support and total L
. S e motivation
operational suitability are demonstrated.
T Transmission Z’Ilir;ualorautomatlc, matched by the OEM to the drivetrain and operating OEM data sheet
Not less than 230 mm at the manufacturer-designated
T6 Ground clearance measurement point, excluding removable steps or mud flaps. OEM data sheet
Bidder to state.
Minimum 1 000 kg payload, calculated after standard equipment.
T7 Payload Final available payload after the mandatory tow-bar installation Mass calculation and OEM data
shall be declared.
. OEM-rated braked towing capacity of at least 2 500 kg. Unbraked capacity, . -
T8 Towing tow-ball limit and GCM shall be stated. OEM towing certificate/data
To Fuel capacity/range B@der to state tank gapamty and estimated operating range. Vehicle shall be OEM data sheet
suitable for remote field deployment.
Heavy-duty all-terrain tyres of identical make, model and size on all
T10 Tyres road wheels, with appropriate load and speed ratings; one full-size | Tyre specification
spare wheel.
. The exterior colour shall be strictly solid white. No alternative colour, metallic | OEM colour specification and
T11 Exterior colour . o A . X K .
finish, two-tone finish or colour substitution will be accepted. supplier confirmation
- Authorised servicing, warranty and parts support available in South Africa. . .
Uik S ReRETI Bidder shall provide support footprint relevant to delivery areas. Dl EHRERIED (SRS

7.2 Standard equipment

air conditioning and heating;

power steering;

remote or central locking;

OEM immobiliser and alarm or equivalent anti-theft protection;
Bluetooth-capable audio/communication system;

Standard radio (OEM)

driver information display with warning indicators;

front and rear mud flaps where compatible with vehicle design;
full-size spare wheel, jack, wheel spanner and vehicle tool kit;

two compliant warning triangles;

front and rear recovery points rated or approved by the OEM;
daytime running lights where standard, and compliant road lighting;
rear window demister for enclosed rear cab glazing where applicable.
Park Distance Control (PDC)

7.3 Off-road and durability requirements

The offered vehicle shall be suitable for routine use on gravel roads, uneven tracks, servitudes and construction sites. The bidder shall state the
following without exaggeration or unsupported assumptions: approach angle, departure angle, ramp-over angle, wading depth, turning circle,
front and rear axle ratings, wheelbase, track width, ground clearance, tyre specification, differential-lock or traction-management functionality,
and underbody protection fitted as standard or offered. All vehicles offered shall be heavy-duty single-cab 4x4 LDVs intended for demanding
commercial and field operations.

8. SAFETY REQUIREMENTS

Area Mandatory requirement

Three-point seat belts for all outboard seating positions; compliant restraints for every designated seat; head

Occupant restraint . X
P restraints where applicable.

Airbags At least driver and front passenger airbags. Bidder shall state total airbag count and locations.

Braking ABS and electronic brake-force distribution or equivalent OEM system.

Stability Electronic stabilit}/ control and.traction control, unless the bidder prqvifies'evidt.epce that the particular legally
homologated vehicle category is exempt and Eskom accepts the deviation in writing.

Visibility Compliant mirrors, windscreen wipers/washers, reversing lights, high-mounted stop lamp where applicable, and

laminated windscreen.

Audible reverse alarm fitted without interfering with OEM electrical systems or warranty. Rear parking sensors or

Reversing safet e s
g Y camera where specified in the purchase order.

Emergency equipment Two warning triangles and a suitable fire extinguisher securely mounted if instructed.
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® Eskom

The tow-bar installation shall not obstruct sensors, lights, crumple zones, number plates, service access or legal

Tow-bar installation integrity markings

Park Distance Control (PDC) A parking sensor system that helps drivers detect nearby obstacles

9. TOW-BAR REQUIREMENTS

Every vehicle shall be supplied with a heavy-duty tow bar as a mandatory requirement.

Requirement Minimum acceptance criterion

Compatibility OEM-approved or OEM-compatible tow bar designed and rated for the offered vehicle.

Configuration Tow ball or pintle configuration as stated in the purchase order.

Safety provisions Rated safety-chain attachment points and a compliant electrical connection socket.

Certification Permanent rating plate and documentary evidence of the tow-bar rating and installation.

Warranty Installation shall comply with OEM requirements and shall not invalidate or reduce the vehicle warranty.

Inspection Installation shall be secure, correctly aligned, corrosion-protected and free from interference with
vehicle systems or legal markings.

10. DELIVERY, REGISTRATION AND HANDOVER

10.1 Delivery condition

fully assembled and clean;

free from damage, defects, warning lights, fluid leaks and abnormal noise;

licensed, registered and fitted with number plates;

roadworthy and ready forimmediate use;

supplied with the specified tow bar and standard vehicle equipment;

supplied with at least one-quarter tank of fuel, unless otherwise stated in the purchase order;

odometer reading not exceeding 200 km unless Eskom has approved additional distance for fitment, testing or delivery.

10.2 Handover pack

vehicle invoice and delivery note;

registration and licensing documents;

OEM owner’s manual and electronic/manual supplements;
warranty and service-plan documents;

PDI report and tow-bar installation quality checklist;

keys, remotes and security codes;

technical data including GVM, GCM, axle limits, payload and towing limits;
tow-bar rating and installation certificate;
completed-vehicle mass and payload statement;

service and breakdown contact details;

signed acceptance checklist.

11. WARRANTY AND AFTER-SALES SUPPORT

The bidder shall state all warranty and support terms clearly. At minimum:

e OEM vehicle warranty shall start no earlier than the date of delivery/registration to Eskom, except where legally or administratively
unavoidable and disclosed;

tow-bar installation shall carry a supplier or manufacturer warranty that does not reduce the base-vehicle warranty;

transport or pre-delivery damage remains the supplier’s responsibility until acceptance;

warranty repairs shall use approved parts and procedures;

the supplier shall coordinate defects involving the base vehicle and tow-bar installation so that Eskom is not required to resolve
responsibility disputes;

parts availability, roadside assistance, service intervals and turnaround escalation contacts shall be declared;

e recalls, safety campaigns and material technical notices affecting delivered vehicles shall be communicated in writing.

Warranty item Bidder to complete

Base-vehicle warranty Period / distance / conditions

Roadside assistance Coverage and contact details

Tow-bar installation warranty Period and exclusions

Parts support Local availability and lead-time escalation
Warranty network Authorised facilities relevant to operational area
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® E€skom

12. TRAINING

The supplier shall provide brief handover training, at no additional cost, covering safe vehicle and 4x4 operation, payload and towing limits, tow-
bar safety, routine inspections, service intervals and warranty conditions. Attendance shall be confirmed on a signed training checklist.

13. PRICING AND ORDERING

Pricing shall be transparent and separately identify the base vehicle, each optional fitment, licensing/registration, delivery, training and any other
charge. Prices shall be quoted in South African rand and shall state VAT treatment. Eskom will issue purchase orders specifying quantities,
categories, delivery locations and selected options.

The bidder shall disclose assumptions, exclusions, price-validity periods, model-year implications and any volume-dependent conditions. No
unapproved accessory, premium, administration fee or substitution may be added after purchase-order acceptance.
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Specification.pdf
1. INTRODUCTION

Eskom SOC LTD Distribution Gauteng Cluster requires supply of 42 Trucks. These trucks operate
across all Distribution Gauteng Cluster. The vehicles are stationed at various Maintenance and
Operations sites & Support Functions.

2. DEFINITIONS AND TERMINOLOGY

Definition

Explanation

Ancillary equipment

Any item purchased and fitted to a vehicle, which is not fitted as
original equipment by the vehicle manufacturer

Accessory equipment

Accessory equipment are "add-ons" a carrier can install on the
vehicle to improve efficiency, safety, comfort, or ease of operation.

Under-run protection
devices

Side under-run protection devices or "lateral protection devices"
occupy larger spaces between axles on a rigid truck or a semitrailer.
They are barriers or plates that sit in the space between axles.
They are designed for the following purposes:
1. To stop other road users such as other vehicles, cyclists, and
pedestrians getting under the rear wheels of a truck or trailer.
2. To minimise the potential damage a roadside obstacle might
cause if the truck turns in too early.

Heavy vehicle (trucks
or yellow plant)

A vehicle with a gross vehicle mass of more than 3 500 kg.

Heavy axle" means an axle whose wheels are fitted with tyres of a
size (bead seat diameter) greater than 406.4 mm (16 inches), or an
axle with more than two wheels regardless of tyre size, but excluding
any axle of a motorcycle, a motor tricycle, or a motor car.

'Heavy vehicle" means a motor vehicle with at least one heavy

axle and/or any vehicle that has been principally designed or

adapted for the convenience of persons exceeding 16 in number.






3. ABBREVIATION

Abbreviation Explanation
LDV Light delivery vehicle

NRTA National road traffic act

SRS Supplemental restraint system

LWB Low Wheelbase

SWB Short Wheelbase

HGC High ground clearance

ABS Antl-Lock braking system

BEV Battery electric vehicle

EV Electric vehicle

BU Business unit

GVM Gross vehicle mass

ISO International organization for standardization
LDV Light delivery vehicle

LWB Long wheelbase

NRTA National road traffic act

OBD/II Onboard diagnostic second-generation
RTM Act Road traffic management act.

VMD Vehicle-monitoring device

A&F Assurance and forensic department
RMI Retail motor industry

SANS South African national standards

4. APPLICABLE LAWS AND LEGISLATIONS

[1] SANS 1563 — The strength of large passenger vehicle superstructures (Rollover protection)

[2] 1SO 9001 Quality management systems

[3] ISO 45001 Occupational health and safety






[4] National Road Traffic Act 93 of 1996
[5] National Environmental Management: Air Quality Act No 39 of 2004

5. SCOPE OF WORK

The supply and delivery of various class of trucks to Distribution Gauteng Cluster on a as and
when required basis for period of 3 years. The bid is for the supply, delivery, licensed, fuelled
and hand over of the fleet in perfect working order and ready for immediate use on public and
rural roads. The vehicles shall be designed for and be capable of efficient and safe operation
under all South African weather conditions.

5.1 VEHICLE CATEGORIES

TAAD Light Truck 4x4 GVM (Dual wheel application)

T5AD Medium Truck 4x4 > 13000 <16000 GVM (Dual wheel application)
T5AS Medium Truck 4x4 >13000 <16000 GVM (Single wheel application)
T5BD Medium Truck 4x4 > 16000 < 19000GVM (Dual wheel application)
Til Heavy Truck 6x6 26000 GCM (Single Wheel application)

Eskom reserves the right to order vehicles on an as-and-when required basis during the contract
period. By virtue of being appointed as one of the successful suppliers does not entitle the
supplier to impose the placing of orders to the full value at any given time during the contract

period.

6. TECHNICAL SPECIFICATION/DETAILED SCOPE OF WORK

6.1 STANDARD REQUIREMENTS

All commercial vehicles shall comply with the provisions of the National Road
Traffic Act, as amended

Vehicle tools required to be supplied with the vehicle shall consist of at least a
suitable jack handle, wheel nut spanner and 2x emergency warning signs triangle
and/or cones).

A spare wheel must be supplied with the provision to permanently mount the
spare

All vehicles must be supplied with front and rear backing plates for the fitment of
number plates.

All vehicles that require Road Worthy Certificates should be supplied with mass
plates affixed to the vehicle.





All vehicles that require Road Worthy Certificates should be supplied with all
accessories, fitment and signage as required (e.g. fire extinguisher, seating

capacity, speed limitation sign and conspicuity tape)

The following categories of vehicles must be supplied standard as a minimum, as
provided below: Commercial vehicle specifications - gross vehicle mass (GVM) 3
500 kg and above (including heavy commercial vehicles with GVM above 16 000

kg and abnormal vehicles):

LR NOURWNE

18.

19.

20.

21.

22.

Radio/ MP3 player/blue tooth
Central locking system

Power steering

Fog lights

Immobiliser

Alarm

Air Conditioner
Driver and passenger airbags.

ABS braking system.

Daytime running lights

Seat Belts: SABS approved

Factory-fitted power steering

Reverse lights

Reverse alarm / beeper

Driver and passenger seatbelt reminder/alarm

Head light on reminder indicator/alarm when vehicle is
switch off

All seats are to be covered with a durable fabric and fitted

with headrests

Yellow reflective tape that must be fitted in accordance with the
National Road Traffic Act specification xix. Anti-spray mudflaps xx.
Under-run protection device in accordance with the SANS 1055
standards

Chevron warning plates in accordance with the National Road
Traffic Act specification xxii. A speed limit warning sign in
accordance with the National Road Traffic Act specification.

Any other apparatus (including large toolboxes) shall be fitted in
such a manner that it would be sufficiently secured in the event
of vehicle rollover or collision and would not create a risk by
weakening the structure of the vehicle.

Applicable warning signs for the type of transportation should be

fitted in accordance with legislation.

Homologation of load body according to (Road traffic Act and

Regulations No. 192A)





23.  Allowances must be made on the load body sizes of relevant LDV's
and trucks for additional fitments to the trucks such as cranes,
hydraulic platforms (cherry pickers), etc. to ensure that the fitment
of the accessories and the load body of the fleet item is compatible
with the chassis of the fleet item

6.2 TABLE OF VEHICLE CATEGORIES

Category Description Code

Truck 4x4 FIC
Light Truck 4x4 D 4x4 >4500 < 7000 kg D/Wheel TA4AD
Medium Truck 4x4 >13000 < 16000 kg, GVM D/Wheel T5AD
Medium Truck 4x4 >13000 < 16000 kg, GVM S/Wheel T5AS
Medium Truck 4x4 > 16000 < 19000 kg, GVM D/Wheel T5BD

Extra heavy Truck 6x6
Extra Heavy Truck 6x6 > 26000 kg, GVM & above Til

Category "T4AD" Light Truck 4x4 > 4500 < 7000 kq (Dual wheel application)

Vehicle Job Required for carrying goods, equipment and passengers up to a GVM of|
Description | 7000 kg on all types of road surfaces with up to 80 % off road usage.

(Licence code Cl)






Technical
Specification

kW output: Minimum 100 kW
Nm torque: Minimum 350 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating "2600 kg to 2800kg"
Permissible rear axle rating "4300 kg 6000kg"
DIT rating: " max 7000 kg"
Wheelbase: "3365 mm to 4000 mm
Air conditioner factory fitted
Driver and passenger airbags
Driver and passenger seatbelt reminder indicator / alarm
Daytime run lights
ABS brakes
Power steering
Radio/ MP3 player/blue tooth
Two emergency triangles
Rear overhang: Not to exceed 50 % of wheelbase
Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system
Trailer brake control (optional)
Fitted towing/recovery facility on front
Tyre (Size), As per manufacture 7.50R16-10 PR (up to 80% off road
_usage) Compatible diff-ratio.
Noise Level: Not to exceed 75db
Colour: White
Reverse alarm / beeper

Permitted
accessory’s

Truck mounted crane, 6 Ton metre range
Tail lift 1.5 Ton capacity
1 1m round to bottom of basket aerial platform Live line SSI






Permitted
ancillaries are
optional

Tow bar

Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's
gearbox is engaged (or hand-brake failsafe system / alarm) (in any
gear).

Flatbed drop side

Cargo van body

Tool cab

Ladder rack

"H" frame

Toolboxes

Stainless steel water tank

Working lights

Amber revolving light

Under run bumper fixed or energy absorbing type

Wheel Flaps: SABS 1496 specification

Yellow reflective tape that must be fitted (Road traffic act and
regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations No. 192A)

Medium Truck 4x4 > 13000 < 16000 kq GVM

Category "T5AS" Single rear tyres (Single - 12R 20 Tyres)

Vehicle Job |Required for carrying goods, equipment, and passengers up to a GVM of
Description 116000 kg on all types of road surfaces with up to 80 % off road usage.






Technical
Specification

kW output: Minimum 170 kW

Nm torque: Minimum 750 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating "4700kg to 5500kg"
Permissible rear axle rating "max 8000 kg" single rear wheels
D/T rating: "17500 to 21000kg"

Wheelbase: "3900mm to 4800mm"

Air conditioner factory fitted

Driver and passenger airbags

Dat time running light

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Rear overhang: Not to exceed 50 % of wheelbase
Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system
Trailer brake control (optional)

Fitted towing/recovery facility on front

Tyres: As per manufactures specifications (Single rear tyres - 12R 20)
Noise Level: not to exceed 75db

Reverse alarm / beeper

Permitted
accessory’s

Truck mounted crane, 13 Ton metre range
Tail lift 2-Ton capacity
15m round to bottom of basket aerial platform Live line SSI






Permitted ow bar
ancillaries are Air conditioner
optional Hour meter
Interlock hand brake system
PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's gearbox
is engaged (or hand-brake failsafe system / alarm) (in any gear). Flatbed
drop side cargo van body
Tool Cab
Ladder rack frame
Toolboxes
Stainless steel water tank
Working lights
Amber revolving light
Under run bumper fixed or energy absorbing type
Wheel Fla s: SABS 1496 specification
Boor Machine
Air charge line to front and rear & coupling

Yellow reflective tape that must be fitted. (Road traffic Act and Regulations
No. 192A)

Homologation of load body according to (Road traffic Act and Regulations
No. 192A
Medium Truck 4x4 > 13000 < 16000 kq GVM

Category "T5AD" (Dual rear tyres)

Vehicle Job Required for carrying Goods, equipment, and passengers up to a GVM of
Description 16000 kg on all types of road surfaces with up to 80 % off road usage,






Technical
Specification

KW output: Minimum 170kw

Torque: Minimum 706Nm to 810Nm

Diesel Powered (Normally aspirated or Turbo)
Permissible Front axle Rating "4700kg to 5500kg 'i
Permissible Rear axle Rating "max 8000 kg" single rear wheels
D/T Rating: "17500 to 21000kg"

Wheelbase: "3900mm to 4800mm"

Air Conditioner Factory fitted

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Two emergency triangles

Rear Overhang: Not to exceed 50 % of wheelbase
Manufactures approved Engine Protection Device
Chassis to facilitate the fitting of hydraulic crane

Fully Synchromesh Gearbox with transfer box (4x4)
Brakes to be air assisted or full air dual system

Trailer brake control (optional)

Fitted towing/recovery facility on front

Tyres: As per Manufactures Specifications (Single rear tyres - 12R 20)

Noise Level: not to exceed 75db
Reverse alarm / bee

Permitted
accessory's

Truck Mounted Crane, 13 Ton Metre range
Tail lift 2-ton capacity
15m round to bottom of basket Aerial platform Live line SSI






Permitted
ancillaries are
optional

Tow bar

Air conditioner

Hour meter

Interlock hand brake system

PTO

Flat Bed Drop side

Cargo van body

Tool cab

Ladder Rack

H" Frame

Toolboxes

Stainless steel Water Tank

Working Lights

Amber Revolving Light

Under run bumper fixed or energy absorbing type
Wheel Flaps: SABS 1496 specification Boor Machine
Air charge line to front and rear & coupling.

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations

No. 192A

Medium Truck 4x4 > 16000 < 19000 kg GVM

Category "T5BD" Dual rear tyres -T5BD

Vehicle Job
Description

Required for carrying goods, equipment and passengers up to a GVM of
19000 kg. On all types of road surfaces with up to 80 % off road usage.






Technical
Specification

kW output: Minimum 170 kW Nm
torque: Minimum 810 Nm

Diesel powered (Normally aspirated or turbo)
Permissible front axle rating 17100kg to 7700kg"
Permissible rear axle rating "9000 kg"

D/T rating: " 28000 kg"

Wheelbase: "Minimum 4500 mm and 4800 maximum"
Rear overhang: Not to exceed 50 % of wheelbase

Air conditioner factory fitted

Day time running light

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm
Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Chassis to facilitate the fitting of hydraulic crane front or rear mounted
Fully synchromesh gearbox with manual shift /automatic gearbox.
Gear ratio: Top gear 1 :1 and Lowest gear higher than 8:1

Top speed of vehicle max 100kmph (determine by gear ratio, no
electronic speed limiters allowed)

Independent transfer box (4x4)

Diff ratios to be determined by top speed of vehicle Trailer brake control
Fitted towing/recovery facility on front

Tyres: As per manufactures specifications Noise Level: not to exceed
75db

Reverse alarm / beeper

Permitted
accessory's

Truck mounted crane, 16 Ton metre range.
HHH / DTH drilling rig (With compressor separately)
15m round to bottom of basket aerial platform Live line OCI






Permitted Tow bar

ancillaries are Air conditioner

optional Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or mechanical
interlock to disallow the PTO from operating while the vehicle's gearbox
is engaged (or hand-brake failsafe system / alarm) (in any gear). Flatbed
drop side / Cargo van body Ladder rack

“H” frame

Toolboxes

Stainless steel water tank

Working lights

Amber revolving light

Under run bumper fixed or energy absorbing type

Wheel flaps: SABS 1496 specification

Air charge line to front and rear & coupling

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Regulations No. 192A)

Extra Heavy Truck 6x6 > 26000 kq GVM & above

Category "T11 "(Dual rear tyres or Single rear tyres)

Vehicle Job Required for carrying goods & equipment of up to 75000 kg GCM on all types
Description of road surfaces short & long distance. (Licence code ECI)






Technical
Specification

kW output: Minimum 300

kW Nm torque: Minimum

1500 Nm

Diesel powered (Normally aspirated or turbo)

Permissible front axle rating "max 8000 kg'

Permissible rear axle rating "max 16000kg single and 18000kg
dual" D/T rating: "max 56000 kg"

Wheelbase: (Centre front axle to centre of rear axle unit) 4525mm
Air conditioner factory fitted

Daytime running lights

Driver and passenger airbags

Driver and passenger seatbelt reminder indicator / alarm

Head light reminder indicator/alarm

ABS brakes

Power steering

Radio/ MP3 player/blue tooth

Two emergency triangles

Manufactures approved engine protection device
Chassis to facilitate the fitting of hydraulic crane
Fully synchromesh

Brakes to be air assisted or full air dual system
Trailer brake control

Fitted towing/recovery facility on front

5th wheel manufactures approved.

Tyres: As per manufactures specifications (Tredco)
Noise Level: Not to exceed 75db

Reverse alarm / beeper

Permitted
accessory's

Truck mounted crane max 22 Ton metre range
25 M bottom to basket OCI, SSI aerial platform

Permitted
ancillaries are
optional

Air conditioner

Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or
mechanical interlock to disallow the PTO from operating while the
vehicle's gearbox is engaged (or hand-brake failsafe system / alarm)
(in any gear).

Toolboxes

Working lights

Amber revolving light

Wheel flaps: SABS 1496 specification

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No,192A






Fitted towing/recovery facility on front
5" wheel manufactures approved.

Tyres: As per manufactures specifications
(Tredco) Noise Level: Not to exceed 75db
Reverse alarm / bee er

Permitted Truck mounted crane max 22 Ton metre range
accessory’s 25 M bottom to basket OCI, SSI aerial platform
Permitted Air conditioner

Ancillaries Hour meter

Interlock hand brake system

PTO -Where a PTO is utilised there should be an electric or
mechanical interlock to disallow the PTO from operating while the
vehicle's gearbox is engaged (or hand-brake failsafe system / alarm)
(in any gear). Toolboxes

Working lights

Amber revolving light

Wheel flaps: SABS 1496 specification

Yellow reflective tape that must be fitted. (Road traffic Act and
Regulations No. 192A)

Homologation of load body according to (Road traffic Act and
Re illations No. 192A

6.2 MODEL CHANGE

e Any known model changes/enhancements may be stipulated by bidders in the bid
response and accommodated in the item's price stipulated upfront in the pricing
Schedule. Thus, price changes due to model changes/enhancements will not be
accepted post the award of the contract.

e Should a vehicle model or shape change (or facelift) the new model should either
be offered under the same price as the previous model or as a separate item at the
time of bid submission or resubmission of pricing process.

e When offering it as a separate item, the bidder must indicate the date at which the
model change will become effective as well as the date when the old model will no
longer be available.

e Model changes/enhancements that are offered to Eskom at no additional cost must
remain within the same vehicle category as the original item offered.

6.3 VEHICLE REGISTRATION AND LICENSING

The service provider will be responsible for registration and licensing of the vehicles.





6.4 WARRANTEES/GUARANTEES

e All vehicles supplied in terms of this contract are required to have a
warrantee/guarantee which is to be effective on the date that Eskom take possession
of the vehicle.

e The warrantee/guarantee must be valid in accordance with the manufacturing
standards of the vehicle as stated by the manufacturer.

e Full details of the vehicle warranties/guaranties must be provided electronically and
printed as part of the bid submission.

e The service provider guarantees that the items supplied under the contract are new
and unused.

e The insurance of items against loss or damage incidental to manufacture or
acquisition, transportation, storage and delivery will be the responsibility of the
service provider. Any damaged parts of the vehicle because of manufacture or
acquisition, transportation, storage and delivery must be replaced with new and
unused parts.

Eskom must be informed if the ordered vehicle is damaged while in transit.
Eskom retains the right to take delivery or refuse to take delivery of any vehicle once
it was damaged.

e Eskom will not take possession of any vehicle exceeding 200km on the odometer of
the vehicle at the time of delivery, unless such vehicle needed to be moved for
conversion or the fitment of accessories.

e The successful bidder will be required to provide Eskom with documentation or
certification confirming the warrantee, service plan and maintenance plan.

6.5TRAINING

e Hand-over training or vehicle orientation is required when vehicles are delivered
this will include the training of individuals to operate a specific vehicle and all accessories
thereto safely, economically and effectively.

e Hand-over training will have to be provided for a minimum of two officials as identified by
Eskom at the time of delivery of the vehicle at no additional cost to Eskom.
The service provider can make available pre-arranged group sessions for the
introduction of the new vehicle models.

e Any service provider on the contract will need to train up any individual that is
identified by Eskom for the operation of any vehicle supplied on the contract at
no additional cost.
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SCOPE OF WORK

SUPPLY, DELIVERY, REGISTRATION AND SUPPORT OF HEAVY-DUTY SINGLE-CAB 4x4 LIGHT DELIVERY VEHICLES
Brand-neutral, performance-based procurement specification

® E€skom

Do e d D
Business unit Eskom Distribution
Operational area Gauteng Cluster and other Eskom operations, as instructed
Contract basis As and when required
Vehicle class New heavy-duty single-cab 4x4 Light Delivery Vehicles (LDVs)
Prepared by Vuyokazi Maseti
Status Draft for review and approval
Document date 09 September 2026

IMPORTANT

No make, brand, model or country of origin is prescribed. Any compliant vehicle may be offered, provided it meets every mandatory functional,
safety, legal, technical, warranty and support requirement in this Scope of Work.

ABSTRACT

This document defines the requirements for the supply, delivery, licensing, registration, fitment, handover, warranty of new heavy-duty single-
cab 4x4 Light Delivery Vehicles for Eskom operational use for a period of three years. The specification is deliberately brand-neutral and
outcome-based to promote fair competition while ensuring that vehicles are safe, durable, serviceable and suitable for demanding on-road and
off-road conditions.

CONFIGURATION CONTROL

0 09 September 2026 Vuyokazi Maseti Recreated as a brand-neutral 4x4 LDV Scope of Work
Actio ame Designatio gnature Date
Compiled Vuyokazi Maseti Fleet Manager - Gauteng Cluster e 09.09.2026
Reviewed ( N
Sl & b
Approved Xolile Mlaba Senior Manager Gauteng (Acting) \M\(&}‘h 09/09/2026

1. INTRODUCTION

Eskom requires heavy-duty single-cab 4x4 LDVs to support field activities in rural areas, construction and maintenance sites, distribution
network servitudes, gravel roads, agricultural and mining environments, remote locations and emergency-response operations. Vehicles may be
used for transporting employees, tools and equipment under variable road and weather conditions.

The procurement shall not be restricted to a particular manufacturer. The supplier may offer any make and model that is commercially available
in South Africa and that fully satisfies the mandatory requirements and provides adequate national or regional support.

2. PURPOSE AND OBIJECTIVES

The purpose of this Scope of Work is to appoint minimum of one and maximum of four capable suppliers to provide new heavy-duty single-cab
4x4 LDVs on an as-and-when-required basis for a period of three years. The objectives are to:
e obtain fit-for-purpose vehicles through fair, brand-neutral competition;
ensure legal compliance, roadworthiness and occupant safety;
provide dependable off-road mobility, payload and towing capability;
secure predictable warranty, servicing, parts and technical support;
standardise minimum tow-bar installation and documentation without prescribing a proprietary platform;
apply measurable inspection and acceptance criteria at delivery.
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3. DEFINITIONS AND ABBREVIATIONS

SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

A drivetrain capable of supplying driving force to all four wheels, with driver-selectable or automatic four-wheel-

4x4/4WD drive functionality suitable for off-road use.

LDV A Light Delivery Vehicle configured exclusively as a single-cab pickup and specified for heavy-duty
commercial and field operations.

OEM Original Equipment Manufacturer.

Supplier The contracted party responsible for the complete supply, fitment, delivery, documentation and support

obligation.

Mandatory requirement

Arequirement that must be met. A material failure may render an offer technically unacceptable.

GVM

Gross Vehicle Mass stated by the OEM.

GCM Gross Combination Mass stated by the OEM.

Payload Eermissible carrying capacity calculated and declared in accordance with the OEM specification and legal
limits.

PDI Pre-delivery inspection.

SANS South African National Standards.

NRTA National Road Traffic Act 93 of 1996 and applicable regulations.

PDC Park Distance Control

4. APPLICABLE LEGISLATION AND STANDARDS

At the time of delivery, each vehicle and all tow-bar installation shall comply with applicable South African legal and regulatory requirements. The
supplier shall identify the exact standards and approvals applicable to the offered vehicle. These include, where applicable:
National Road Traffic Act 93 of 1996 and regulations;
South African vehicle homologation and certification requirements;
applicable SANS requirements for vehicles, components, glazing, lighting, tyres, towing equipment and electrical tow-bar installation;
Occupational Health and Safety Act 85 of 1993 where work, fitment or handover activities are performed;
National Environmental Management Act 107 of 1998 and applicable emissions requirements;

e OEM manufacturing, body-builder, loading, towing, fitment and warranty instructions.
Where a cited standard is revised, the version legally applicable at the date of manufacture or delivery shall apply, unless Eskom specifies
otherwise in the purchase order.

5. SCOPE OF SUPPLY

The supplier shall provide a complete, operational and road-legal vehicle solution. The scope includes:
sourcing and supplying new, unused 4x4 LDVs;

all specified standard vehicle equipment;

PDI, quality checks and roadworthiness confirmation;

registration, licensing and number plates in the nominated Eskom entity name;

fuel sufficient for handover and operational movement;

delivery to the location stated in each purchase order;

handover documentation, keys, manuals and training;

warranty, service support, parts support and defect rectification.

Quantities, cab configuration, delivery location and optional tow-bar installation will be stated in individual purchase orders. No minimum
volume is guaranteed unless expressly stated in the contract.

6. VEHICLE CATEGORIES

Category

Intended use

Minimum configuration

Category A: Heavy-Duty
Single-Cab 4x4 LDV

Tools, equipment, field maintenance and payload-
focused operations

Two-door single-cab pickup; seating for at least two
occupants; load box.

7. TECHNICAL AND FUNCTIONAL REQUIREMENTS

7.1 Core vehicle requirements

Ref. Requirement Minimum acceptance criterion Bidder evidence
- Factory-new, unused, current production vehicle; not previously registered OEM specification and supplier
T Condition A X - X .
except where required for delivery administration. declaration
Heavy-duty single-cab LDV/pickup with a separate load box and
T2 Body type . . . Brochure/data sheet
commercial-duty chassis construction.
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SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

Ref. Requirement Minimum acceptance criterion Bidder evidence
Functional 4x4/4WD system suitable for low-traction and off-road conditions.
T3 Drivetrain Where low range is not fitted, bidder shall demonstrate equivalent off-road OEM technical data
capability.
) Dlesel.preferred-. Alterna?lveApowertram may pe offered only if range, Technical schedule and
T4 Engine refuelling/charging practicality, payload, towing, support and total L
. S e motivation
operational suitability are demonstrated.
T Transmission Z’Ilir;ualorautomatlc, matched by the OEM to the drivetrain and operating OEM data sheet
Not less than 230 mm at the manufacturer-designated
T6 Ground clearance measurement point, excluding removable steps or mud flaps. OEM data sheet
Bidder to state.
Minimum 1 000 kg payload, calculated after standard equipment.
T7 Payload Final available payload after the mandatory tow-bar installation Mass calculation and OEM data
shall be declared.
. OEM-rated braked towing capacity of at least 2 500 kg. Unbraked capacity, . -
T8 Towing tow-ball limit and GCM shall be stated. OEM towing certificate/data
To Fuel capacity/range B@der to state tank gapamty and estimated operating range. Vehicle shall be OEM data sheet
suitable for remote field deployment.
Heavy-duty all-terrain tyres of identical make, model and size on all
T10 Tyres road wheels, with appropriate load and speed ratings; one full-size | Tyre specification
spare wheel.
. The exterior colour shall be strictly solid white. No alternative colour, metallic | OEM colour specification and
T11 Exterior colour . o A . X K .
finish, two-tone finish or colour substitution will be accepted. supplier confirmation
- Authorised servicing, warranty and parts support available in South Africa. . .
Uik S ReRETI Bidder shall provide support footprint relevant to delivery areas. Dl EHRERIED (SRS

7.2 Standard equipment

air conditioning and heating;

power steering;

remote or central locking;

OEM immobiliser and alarm or equivalent anti-theft protection;
Bluetooth-capable audio/communication system;

Standard radio (OEM)

driver information display with warning indicators;

front and rear mud flaps where compatible with vehicle design;
full-size spare wheel, jack, wheel spanner and vehicle tool kit;

two compliant warning triangles;

front and rear recovery points rated or approved by the OEM;
daytime running lights where standard, and compliant road lighting;
rear window demister for enclosed rear cab glazing where applicable.
Park Distance Control (PDC)

7.3 Off-road and durability requirements

The offered vehicle shall be suitable for routine use on gravel roads, uneven tracks, servitudes and construction sites. The bidder shall state the
following without exaggeration or unsupported assumptions: approach angle, departure angle, ramp-over angle, wading depth, turning circle,
front and rear axle ratings, wheelbase, track width, ground clearance, tyre specification, differential-lock or traction-management functionality,
and underbody protection fitted as standard or offered. All vehicles offered shall be heavy-duty single-cab 4x4 LDVs intended for demanding
commercial and field operations.

8. SAFETY REQUIREMENTS

Area Mandatory requirement

Three-point seat belts for all outboard seating positions; compliant restraints for every designated seat; head

Occupant restraint . X
P restraints where applicable.

Airbags At least driver and front passenger airbags. Bidder shall state total airbag count and locations.

Braking ABS and electronic brake-force distribution or equivalent OEM system.

Stability Electronic stabilit}/ control and.traction control, unless the bidder prqvifies'evidt.epce that the particular legally
homologated vehicle category is exempt and Eskom accepts the deviation in writing.

Visibility Compliant mirrors, windscreen wipers/washers, reversing lights, high-mounted stop lamp where applicable, and

laminated windscreen.

Audible reverse alarm fitted without interfering with OEM electrical systems or warranty. Rear parking sensors or

Reversing safet e s
g Y camera where specified in the purchase order.

Emergency equipment Two warning triangles and a suitable fire extinguisher securely mounted if instructed.
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SCOPE OF WORK | SUPPLY AND DELIVERY OF 4x4 LIGHT DELIVERY VEHICLES

® Eskom

The tow-bar installation shall not obstruct sensors, lights, crumple zones, number plates, service access or legal

Tow-bar installation integrity markings

Park Distance Control (PDC) A parking sensor system that helps drivers detect nearby obstacles

9. TOW-BAR REQUIREMENTS

Every vehicle shall be supplied with a heavy-duty tow bar as a mandatory requirement.

Requirement Minimum acceptance criterion

Compatibility OEM-approved or OEM-compatible tow bar designed and rated for the offered vehicle.

Configuration Tow ball or pintle configuration as stated in the purchase order.

Safety provisions Rated safety-chain attachment points and a compliant electrical connection socket.

Certification Permanent rating plate and documentary evidence of the tow-bar rating and installation.

Warranty Installation shall comply with OEM requirements and shall not invalidate or reduce the vehicle warranty.

Inspection Installation shall be secure, correctly aligned, corrosion-protected and free from interference with
vehicle systems or legal markings.

10. DELIVERY, REGISTRATION AND HANDOVER

10.1 Delivery condition

fully assembled and clean;

free from damage, defects, warning lights, fluid leaks and abnormal noise;

licensed, registered and fitted with number plates;

roadworthy and ready forimmediate use;

supplied with the specified tow bar and standard vehicle equipment;

supplied with at least one-quarter tank of fuel, unless otherwise stated in the purchase order;

odometer reading not exceeding 200 km unless Eskom has approved additional distance for fitment, testing or delivery.

10.2 Handover pack

vehicle invoice and delivery note;

registration and licensing documents;

OEM owner’s manual and electronic/manual supplements;
warranty and service-plan documents;

PDI report and tow-bar installation quality checklist;

keys, remotes and security codes;

technical data including GVM, GCM, axle limits, payload and towing limits;
tow-bar rating and installation certificate;
completed-vehicle mass and payload statement;

service and breakdown contact details;

signed acceptance checklist.

11. WARRANTY AND AFTER-SALES SUPPORT

The bidder shall state all warranty and support terms clearly. At minimum:

e OEM vehicle warranty shall start no earlier than the date of delivery/registration to Eskom, except where legally or administratively
unavoidable and disclosed;

tow-bar installation shall carry a supplier or manufacturer warranty that does not reduce the base-vehicle warranty;

transport or pre-delivery damage remains the supplier’s responsibility until acceptance;

warranty repairs shall use approved parts and procedures;

the supplier shall coordinate defects involving the base vehicle and tow-bar installation so that Eskom is not required to resolve
responsibility disputes;

parts availability, roadside assistance, service intervals and turnaround escalation contacts shall be declared;

e recalls, safety campaigns and material technical notices affecting delivered vehicles shall be communicated in writing.

Warranty item Bidder to complete

Base-vehicle warranty Period / distance / conditions

Roadside assistance Coverage and contact details

Tow-bar installation warranty Period and exclusions

Parts support Local availability and lead-time escalation
Warranty network Authorised facilities relevant to operational area
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12. TRAINING

The supplier shall provide brief handover training, at no additional cost, covering safe vehicle and 4x4 operation, payload and towing limits, tow-
bar safety, routine inspections, service intervals and warranty conditions. Attendance shall be confirmed on a signed training checklist.

13. PRICING AND ORDERING

Pricing shall be transparent and separately identify the base vehicle, each optional fitment, licensing/registration, delivery, training and any other
charge. Prices shall be quoted in South African rand and shall state VAT treatment. Eskom will issue purchase orders specifying quantities,
categories, delivery locations and selected options.

The bidder shall disclose assumptions, exclusions, price-validity periods, model-year implications and any volume-dependent conditions. No
unapproved accessory, premium, administration fee or substitution may be added after purchase-order acceptance.
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