THE APPOINTMENT OF A PANEL OF ELECTRICAL CONTRACTORS FOR THE PROVISION OF ELECTRICAL MAINTENANCE, REPAIRS, INSTALLATIONS, TESTING, COMMISSIONING AND EMERGENCY SERVICES AS AND WHEN REQUIRED, FOR A PERIOD OF THIRTY-SIX (36) MONTHS.

SCOPE OF WORK
The appointed contractor(s) shall provide all labour, supervision, transport, specialized tools, equipment, consumables, replacement materials (where authorized), and technical expertise necessary to execute electrical maintenance works.
The contractor shall provide a twenty-four (24) hour emergency response service, seven (7) days per week, including weekends and public holidays.
· The contractor shall maintain an emergency telephone number that is always operational.
· Suitably qualified personnel shall be dispatched immediately upon receipt of an emergency call.
· Preventive maintenance schedules shall be agreed upon with the College's Facilities Management Unit.

The scope of work includes, but is not limited to, the following:
5.1	Preventive Maintenance:
· Total loss of electrical supply.
· Electrical faults affecting teaching and learning.
· Tripped main breakers.
· Distribution Board failures.
· Electrical fires.
· Exposed live conductors.
· Damaged underground electrical cables.
· Generator failures.
· UPS failures.
· Failure of emergency lighting.
· High mast lighting failures affecting campus safety.
· Security lighting failures.
· Dangerous electrical installations.
· Flood-damaged electrical systems.
· Storm-related electrical damage.
· Lightning damage.
· Electrical shocks and unsafe conditions.
5.2	 Corrective Maintenance
The appointed contractor(s) shall provide corrective maintenance services to restore electrical systems and equipment to full operational condition following faults, failures, damage, or deterioration.
Corrective maintenance shall include, but shall not be limited to:
· Fault finding and diagnosis of electrical systems.
· Repair or replacement of damaged electrical cables.
· Repair and replacement of defective switches and socket outlets.
· Repair and replacement of lighting fittings, lamps, LED luminaires, floodlights, and high mast lighting.
· Repair or replacement of circuit breakers (MCBs, MCCBs and RCBOs).

· Repair and replacement of earth leakage protection devices.
· Repair and replacement of isolators and disconnect switches.
· Repair of damaged electrical conduits, trunking and cable trays.
· Repair and replacement of electrical distribution boards and associated components.
· Repair and replacement of contactors, relays and timers.
· Repair of generator electrical connections and Automatic Transfer Switches (ATS).
· Repair and replacement of UPS components.
· Repair of electrical motors and motor control circuits.
· Repair of workshop and laboratory electrical installations.
· Repair of outdoor electrical infrastructure.
· Replacement of damaged electrical accessories.
· Restoration of power following electrical failures.
All defective components removed from site shall become the property of the College unless otherwise instructed.
Only new, approved, and SABS-compliant materials shall be used unless otherwise authorised by the Employer.
5.4 	Installation Services
The contractor shall undertake new installations, alterations, upgrades, extensions, and modifications to existing electrical infrastructure.
Installation services shall include, but not be limited to:
· Installation of new electrical reticulation systems.
· Installation of underground and overhead electrical cables.
· Installation of conduits and cable trunking.
· Installation of cable trays and cable ladders.
· Installation of Distribution Boards (DBs).
· Installation of switchgear.
· Installation of isolators.
· Installation of socket outlets and switches.
· Installation of internal lighting systems.
· Installation of external lighting systems.
· Installation of floodlights.
· Installation of high mast lighting.
· Installation of emergency lighting systems.
· Installation of security lighting.
· Installation of standby generator connections.
· Installation of Automatic Transfer Switches (ATS).
· Installation of UPS systems.
· Installation of surge protection devices.
· Installation of lightning protection systems.
· Installation of earthing and bonding systems.
· Installation of electrical control panels.
· Installation of workshop electrical services.
· Installation of laboratory electrical systems.
· Installation of energy-efficient LED lighting.
· Installation of smart lighting controls where required.
· Installation of timer controls and motion sensors.
· Installation of electrical systems for new buildings and renovations.
All electrical installations shall comply fully with the latest editions of:
· SANS 10142-1
· Occupational Health and Safety Act
· Electrical Installation Regulations
· Local Municipal By-Laws
· NRS Standards
· Applicable Eskom Requirements
· Manufacturer Specifications
5.5 	Testing, inspection and commissioning
The contractor shall perform testing and commissioning before any new installation or repaired electrical installation is energised.
Testing shall include, where applicable:
· Insulation resistance testing.
· Earth continuity testing.
· Earth loop impedance testing.
· Earth resistance testing.
· Polarity testing.
· Voltage testing.
· Load testing.
· Functional testing.
· Phase rotation testing.
· Prospective short circuit current testing.
· Residual Current Device (RCD) testing.
· Thermal imaging inspections.
· Generator testing.
· UPS testing.
· Lighting lux level verification.
· Distribution Board testing.
· Protective device coordination checks.
The contractor shall submit all test reports before practical completion of the works.
5.6 	Geysers and Hot Water Systems
The contractor shall undertake:
·  Replacement of heating elements.
·  Replacement of thermostats.
·  Replacement of valves.
· Replacement of vacuum breakers.
· Replacement of temperature and pressure relief valves.
·  Installation of new geysers.
· Repair of geyser leaks.
· Replacement of flexible connectors.
· Maintenance of hot water pipework.
· Electrical connections shall be undertaken only by appropriately qualified personnel where required.



5.7 	Certificates of Compliance (Coc)
Where required by legislation, the appointed contractor shall issue a valid Certificate of Compliance (CoC) for all completed electrical installations, alterations, and additions.
Certificates shall:
· Be issued by a Registered Installation Electrician or Master Installation Electrician.
· Comply with the Electrical Installation Regulations.
· Be signed by the authorised person.
· Include all required test results.
· Be submitted before final payment.
· Be retained by the College for audit purposes.
No installation shall be regarded as complete until the relevant Certificate of Compliance has been submitted and accepted.
5.8 	Emergency Electrical Services
The contractor shall provide a twenty-four (24) hour emergency response service, seven (7) days per week, including weekends and public holidays.
Emergency services shall include, but not be limited to:
· Total loss of electrical supply.
· Electrical faults affecting teaching and learning.
· Tripped main breakers.
· Distribution Board failures.
· Electrical fires.
· Exposed live conductors.
· Damaged underground electrical cables.
· Generator failures.
· UPS failures.
· Failure of emergency lighting.
· High mast lighting failures affecting campus safety.
· Security lighting failures.
· Dangerous electrical installations.
· Flood-damaged electrical systems.
· Storm-related electrical damage.
· Lightning damage.
· Electrical shocks and unsafe conditions.
The contractor shall maintain an emergency telephone number that is operational at all times.
Suitably qualified personnel shall be dispatched immediately upon receipt of an emergency call.
6.  	Deliverables
The appointed contractor(s) shall deliver the following services and documentation throughout the duration of the contract:
6.1 	Maintenance Services
The contractor shall:
· Attend to all authorized electrical work orders.
•	Carry out preventative and corrective maintenance.
•	Complete repairs within the prescribed service levels.
•	Undertake emergency callouts.
•	Perform scheduled inspections.
•	Carry out minor electrical alterations where instructed.
•	Install new electrical infrastructure where approve



















EVALUATION CRITERIA
[bookmark: _Toc146016085]PRE-QUALIFICATION/ADMINISTRATIVE REQUIREMENT
The Pre-qualification/Administrative Information Requirement phase validates the tenderers’ compliance with the legal requirements to conduct business in SA, as well as to specific industry requirement for the supply of services where applicable.
Please see table below for the list of administrative requirements and tick yes if documentation is submitted and no if not submitted.

	Appendix Number
	Description 
of Appendix
	Requirement
	Circle yes
 if submitted

	Appendix A
	RFP Document 
	Each page of the RFP document to be initialled and signed where applicable by a delegated representative
	Yes
	No

	Appendix A1
	Proof of payment
	Attach proof of payment and include the company name and tender reference number.
	Yes
	No

	Appendix B
	Completed technical specifications and pricing
	
Fully complete pricing schedule
	Yes
	No

	Appendix B1
	Mandatory upon Contracting
	Fully signed schedule of Appendix B1
	Yes
	No

	Appendix C
	Confirmation of bank account
	Submit a bank stamped confirmation letter (in case of a JV both parties to submit)
	Yes
	No



	Appendix D
	Company Registration Documents
	Company registration documents (in case of a JV both parties to submit)
	Yes
	No

	Appendix E
	Tax Pin
	An original valid Tax Pin (must be valid on tender closing) (in case of a JV both parties to submit)
	Yes
	No

	Appendix F
	BBBEE certification
	A valid B-BBEE certificate from a SANAS accredited agency or Sworn Affidavit (combined certificate from SANAS)
	Yes
	No

	Appendix G
	Board resolution 
	Attach copy of signed board resolution. Unless sole proprietor
	Yes
	No

	Appendix H
	Declaration of Interest
	Sign the following declarations:
· Point 9 of this tender document 
· SBD 4
· SBD 6.1
· SBD 6.2
	Yes
	No

	Appendix I
	Registration National Treasury (CSD)
	Provide a copy of the full report of registration on National Treasury Central Bidder Database (in case of a JV both parties to submit)
	Yes
	No

	[bookmark: _Hlk205472971]Appendix J
	Financial Statements / Statement of Management Account
	· Recent Audited Financial statements signed by the director and auditors for the last 2 financial years 2024-2025 /Latest) OR
· Statement of Management Account signed by the company director for the last 2 financial years 2024-2025) (in case of a JV both parties to submit)
	Yes
	No



[bookmark: _Hlk238628224]NB: No points will be allocated for this phase. However, bidders who meet the minimum functionality criteria may be afforded an opportunity to submit any outstanding pre-qualification and/or administrative documentation prior to contract award, excluding documents expressly stated in the bid document as mandatory returnable requirements to be submitted by the closing date.


























[bookmark: _Toc146016086]STAGE 1: EVALUATION OF FUNCTIONALITY
Bidders need to obtain a minimum percentage score of 80% and above to progress to the next stage of evaluation.
	FUNCTIONALITY CRITERIA

	POINTS ALLOCATED

	 Proof of Individual and Company registration on the:

· Valid Department of Employment and Labour Electrical Contractor Registration.
· Wireman's Licence.
· Construction Industry Development Board (CIDB) – •	CIDB Grade 2EB or higher.
· No submission
	

= 10 Points

= 10 Points

= 05 Points

= 00 Points 
	


25

	Required qualifications and certifications:

· Electrician with a red seal and / or
· Semi-Skilled Electrician - (RPL / 2-3 years recognised training)
· No submission
	

= 10 Points
= 10 Points

= 00 Points
	

20

	Provide three (3) contactable reference letters on a client letterhead.
· Of similar nature or service for the past (5) years.
· Must have contactable references via telephone and/or email.
· Clearly signed and dated 
· Indicating duration (start to finish) of the contract
3 References verified    
2 References verified   
1 Reference verified 
Reference letter(s) submitted but missing one or more mandatory requirements (letterhead, signature/date, contact details, or contract duration)
  No evidence provided                                                                                                                                                                                                                                                
	








= 15 Points
= 10 Points
= 05 Points
= 02 Points



= 00 Points
	








15

	Proof of ownership / Lease of tools and equipment
· Company Asset register, with a minimum of the following:
· LDV Bakkie: proof of ownership
· Equipment (e.g. Electrical Testing Instruments)
· Power tools and hand tools

· No Submission
	

= 10 Points




= 00 Points
	  


10

	Typical turnaround time / Response Time
· Within 2 hours of a logged call / PO
· Within 3 to 4 hours of a logged call / PO
· Any lead time above 4 hours of a logged call / PO                                          
	
= 10 Points                                                                                                          
= 05 Points 
= 02 Points
	          
           10   



	 
Locality (at least a minimum of 3 from the following as proof that the business is based and operating within the specified locality to score the points allocated:
•	Address on CIPC Documents
•	Address on Banking confirmation letter
•	Address on CSD Registration report
•	Address on SARS correspondence

· Within Sedibeng District Municipality 
· Within Gauteng
· Outside Gauteng                                                                                                      
	                                                                                                            








= 20 Points
= 05 Points
= 02 Points
	
20

	
Total Points
	
100



